These ROMS are for Capcom's Final Fight (1991).
This is a two board set with the following ID's:-
lower CPU: 88617A-7b
upper ROM: 89624B-3

All the ROM board jumpers are set as follows:-
1 IN
2 OUT
3 OUT
4 IN

It looks as if the board can be configured to take standard 27C010's in place
of the Hitachi 16 bit wide PROMS that mine had - all the sockets are there. I
read these as Am27C400's...

FF01-01M BIN       524,288 24/10/96    6:52 <- Hitachi HN62404P
FF03-03M BIN       524,288 24/10/96    6:54 <- Hitachi HN62404P
FF05-05M BIN       524,288 24/10/96    6:55 <- Hitachi HN62404P
FF07-07M BIN       524,288 24/10/96    6:56 <- Hitachi HN62404P
FF32-32M BIN       524,288 24/10/96    6:58 <- Hitachi HN62404P
FF35-42  BIN       131,072 24/10/96    6:59 <- AMD 27C010-175
FF36-43  BIN       131,072 24/10/96    7:00 <- AMD 27C010-175
FF31-37  BIN       131,072 24/10/96    7:01 <- AMD 27C010-175
FF30-36  BIN       131,072 24/10/96    7:02 <- AMD 27C010-175
FF19-19  BIN       131,072 24/10/96    7:02 <- AMD 27C010-175
FF18-18  BIN       131,072 24/10/96    7:03 <- AMD 27C010-175
FF09-09  BIN        65,536 24/10/96    7:04 <- Intel 27512
FF-R11E  BIN           256 24/10/96    7:07 <- AMD AmPAL16L8APC (on ROM board)
FF-R01A  BIN           256 24/10/96    7:08 <- MMI PAL16L8BCN   (on ROM Board)
FF-C12H  BIN           256 24/10/96    7:12 <- MMI PAL16L8ACN   (on CPU board)
FF-C15H  BIN           256 24/10/96    7:12 <- MMI PAL16L8ACN   (on CPU board)
FF-C16H  BIN           256 24/10/96    7:13 <- MMI PAL16L8ACN   (on CPU board)
FF-C12F  BIN           256 24/10/96    7:13 <- MMI PAL16L8ACN   (on CPU board)
FF-C13E  BIN           256 24/10/96    7:14 <- MMI PAL16L8ACN   (on CPU board)
       22 file(s)      3,475,200 bytes

It looks as if all the PALS have their security bit's set preventing reads :(
