=========================================
Have Fun With Our Stuff
Planet_Hemp/us/Padawan/HUMI_USER
Your ToH Team
=========================================

Bugfixes/Changes of ToH3.2:
===========================
- Support for German PayTV cards
- Shifting function for channels in settings
- extended EPG infobar
- extended EPG for some German channels




Bugfixes/Changes of ToH3.1:
===========================
- AC-3 Routine works against DropOuts
- New DiSEqC function to use a DiSEqC switch and up to 4 DiSEqC motors at the same time
- TPS Audio Bugfix
- Pink Plus Bugfix
- Audiobugfix on Audiochannels
- Parserproblem for X-Free fixed
- Bugfix on V+APID (couldn't be changed in PMCT)
- Bugfix to start Portalmode, if the info or time window is open
- PIN input conflict with Portalmode
- Brandnew +CAM-Parser
- CASID from CARD/PMCT
- Bugfixes on Detail Automatic Channel Search (FEC)
- Amos 4°E=Amos 4°W, User 21= User 11
- The DD Option in Direct Portalchannel is fake, MPEG audio is played directly now
- STB Upgrade removed from menu
- You can define macros for following buttons with virtual key code:
  0+RADIO  0x2D
  0+MENU   0x2E
  0+PMINUS 0x2F
  0+PPLUS  0x30
  0+UP     0x31
  0+LEFT   0x32
  0+RIGHT  0x34
  0+DOWN   0x35
  0+ASK    0x37
  0+MUTE   0x38
  0+WHITE  0x39
  0+YELLOW 0x3A
  0+RED    0x3C
  0+GREEN  0x3D
  0+BLUE   0x3E
  0+VPLUS  0x3F
  0+VMINUS 0x36
- Event Reservation Control for Direkt Portal Subchannels
  - switch to channel "Direkt Portal"
  - press red button and then white button
  - input the reservation data
- Additional option in column AutoPID to disable the PCR-PID update: noPCR
- New menu structure
- Many little Bugfixes

Portal-Mode:
------------	
o Event Reservation Control for Direkt Portal Subchannels

  How? 
  1. switch to Direkt Portal
  2. press Red Key
  3. press White Key to do the reservation for subchannels with starting time


+CAM:
-----
o CASID from CARD/PMCT

  With an option in the ToH-Config menu you can control, if the CASID is
  taken from card as normaly or if it should be taken from the PMCT.
  You can do the following selections with the "CAS Preselect":

	CARD|CAS1|CAS2|CAS3|CAS4|CAS5|CAS6

  There are the following new entries in the PMCT:

  CAS1 0000 1800 1762 0500 0100 0B00 4A60
  CAS2 0000 0000 0500 0100 1800 0B00 4A60
  CAS3 0000 0000 0100 1800 0B00 4A60 0000
  CAS4 0000 0000 0500 1800 0B00 4A60 0000
  CAS5 0000 0000 0100 0500 0B00 4A60 0000
  CAS6 0000 0000 0500 0100 1800 0000 0000

  This entries have to be set in the CSV file:

  CAS1 ,0022,0000,1800,1762,0500,0100,0B00,4A60
  CAS2 ,0023,0000,0000,0500,0100,1800,0B00,4A60
  CAS3 ,0024,0000,0000,0100,1800,0B00,4A60,0000
  CAS4 ,0025,0000,0000,0500,1800,0B00,4A60,0000
  CAS5 ,0026,0000,0000,0100,0500,0B00,4A60,0000
  CAS6 ,0027,0000,0000,0500,0100,1800,0000,0000

  After changig the option for CASID, you have to do a CAM reset. (for example 0+RCL)



LNB-Controlling and DiSEqC:
---------------------------
o New DiSEqC function to use a DiSEqC switch and up to 4 DiSEqC motors at the same time

  To use this new feature you have to set the option "Send DiSEqC twice for cascade"
  to "ON" in the ToH-Config menu. 

  If you change to another antenna system ToH3.1 is able to break though 2 cascads.

  Example 1

  5400 -> 0/12V-switch -+-> LNB 
                        |  
                        +-> SG-2100 DiSEqC HH motor  -> LNB




  With ToH3.1 it is possible to control motor systems behind a DiSEQc switch.
  In the orgiginal Humax firmware it is not possible to select DiSEQc A/B/C/D
  when a motor system was set. If "Send DiSEqC twice for cascade" is set to
  "ON", it is possible to add a DiSEQc command for a motor system.


  Example 2

  5400 -> DiSEqC-switch (SUR 210 F)-+-> LNB 
                                    |  
                                    +-> SG-2100 DiSEqC HH motor  -> LNB



  Example 3

  5400 -> DiSEqC-multiswitch(Teka DiSEqC 2.0) ---+-> LNB A 
                                                 |
                                                 +-> SG-2100 DiSEqC HH motor  -> LNB B 
                                                 |
                                                 +-> LNB C 
                                                 |
                                                 +-> LNB D 

  Example 4


            5400 -> optionswitch (SUR 210 F)---+---> | DiSEqC-multiswitch (SMS 9800 NF) +-> LNB A
                                               | +-> |                                  | 
                                               | |                                      +-> LNB B
       5400 -> optionswitch (SUR 210 F)------+-|-+
                                             | +-----------------------------> |                                    
                                             +--> SG-2100 DiSEqC HH motor ---> | DiSEqC-multiswitch (SMS 9800 NF) +-> LNB A (C)


  If u do not need any cascading, you should set "Send DiSEqC twice for cascade" to "OFF".
  But there is one advantage if it is set to "ON", the rotor position is controlled while
  switching on the receiver, to set it to the correct position.
  So you have to try which option is the best for your system.



For Macro Experts:
--------------------------
  Now it is possible to use a "shift key" for macro controlling.
  This "shift key" is done with the 0 key on the remote control.
  The following commands are possible:


  0+RADIO		0x2D
  0+MENU		0x2E
  0+PMINUS		0x2F 
  0+PPLUS		0x30 
  0+UP			0x31
  0+LEFT		0x32
  0+RIGHT		0x34 
  0+DOWN		0x35
  0+ASK			0x37
  0+MUTE		0x38 
  0+WHITE		0x39 
  0+YELLOW		0x3A 
  0+RED			0x3C 
  0+GREEN		0x3D 
  0+BLUE		0x3E 
  0+VPLUS		0x3F 
  0+VMINUS		0x36 
   

DolbyDigital
------------

o AC-3 Routine works against DropOuts

  New Dolby Digital function to remove "DropOuts",
  The AC-3-function done in a new way to remove dropouts on Premiere Direct channels.




Bugfixes/Changes of ToH3.0:
===========================
- Most of ToH menus are converted to original Humax-Menu engine (rest will follow)
- New Config Menu
- Advanced ChannelInfoBox with signal power and signal quality
- New Audio Video User settings
- YUV added to Video formats (a little circuit is needed for YUV)
  (thanx to Cybergent and oldowl from www.beisammen.de)
- Gain adjustment for RGB/YUV
- Format ratio enlarged with Auto 16:9/4:3 function
- Premiere NVOD management function (Portalmode) with yellow key on Portalchannel
- Direct card access mode (to change Premiere PIN from PC or to show user specific data)
- Time Offset (TO) in PMCT reactivated
- New Motor Movement Management
- ChannelInfoBox stays during Movement
- Up to 49 Motor positions available
- Orbital positions with degree-context
- All Satellites with new SatcoDX transponder tables for autoscan 
- New help window with most channel infos
- Option for transparent background picture
- Option to close channellist with OK button
- R/L Audio Option in PMCT to select 2 channel audio films
- Function to repeat DiSEqC command for two times
- O-EPG to get ToH EPG mode
- Pacman

- Most of ToH menus are converted to original Humax-Menu engine (rest will follow)
Most of the ToH style design modules and menus are converted to a common like style.
Some of the ToH menus have still to be converted, it will follow in future versions.

- New Config Menu
There is a new config menu you call it in the ToH entry in main menu, to control most
of the available ToH extended features.

- Advanced ChannelInfoBox with signal power and signal quality
Now in ChannelInfoBox signal power and signal quality is shown and a new symbol if
Portalmode is available on the channel.

- New Audio Video User settings
Since this version it is possible to store three independent Audio Video Setting of
your own. So you can store one mode for using YUV on a projector and one other mode to
use the receiver with a television in RGB or CVBS mode. You can select mode while
pressing blue remote control key (UHF), if you press OK on one selected mode, you can
change A/V Output Settings. All changes are stored in settings.

- YUV is added to Video formats selection (a little circuit is needed for YUV)
With this version there is a direct YUV mode support, you can select it like other
modes (RGB/CVBS/S-Video/YUV). A little circuit is needed to add C-Sync signal to the
Y-Output of the Humax Scart connector. You can see it in the attached picture
Humax_YUV.jpg.

- Gain adjustment for RGB/YUV
It is possible to control and store RGB and YUV gaining with A/V Output Settings.

- Format ratio enlarged with Auto 16:9/4:3 function
All possible Screen Modes can now be controlled with A/V Output Settings.

- Premiere NVOD management function (Portalmode) with yellow key on Portalchannel
A new Portalmode is added to select PPV Subchannels on Premiere. An own documentation
is added for this (see Potalmode.html).

- Direct card access mode, done with Mickey
It's possible to set card commands from PC, for example to set PIN for Premiere cards.
More info will follow in the future.

- Time Offset (TO) in PMCT reactivated
Like in older versions it is possible to activate/deactivate Time Offset function for
special channels with an PMCT entry.

Die DiSEqC Motorsteuerung wurde überarbeitet. Der Null Punkt Rücklauf zu Astra beim Einschalten
wurde entfernt. Ebenfalls wurde die Autofocus Funktion überarbeitet.

- New Motor Movement Management
The DiSEqC motor controlling was done in a new way. The zero movement to Astra during
startup was removed. The lost of focus for motors was worked out.

- ChannelInfoBox stays during Movement
The ChannelInfoBox stays during whole motor movement, to see signal during movement.

- Up to 49 Motor positions available
Now it is possible to store about 49 different satellites positions. The positions with a *
have to be positioned by your own. They are used for an overview.

- Orbital positions with degree-context
All satellites are shown with the correct orbit position also during movement.

- All Satellites with new SatcoDX transponder tables for autoscan 
Transponder list are worked over to scan the right transponders using an autoscan.

- New help window with most channel infos
All useful infos are now shown in the help window by pressing ? on a channel. It can
be scrolled by using cursor up/down.

- Option for transparent background picture
The selection for background pictures was added to get picture transparency. So you can
see how some changes will change the picture in a direct way (for example RGB/YUV gaining).

- Option to close channel list with OK button
Now users can select, if channel list will be closed after pressing OK in the channel list
or it shall work like in older versions. You can control it in Config Menu.

- R/L Audio Option in PMCT to select 2 channel audio films
It is possible to select which audio language shall be active, if a channel shall works as
a 2 channel audio mode channel. It is useful for channels, which sends original audio on
Right and foreign audio on Left channel. You can select with PMCT in ToH EPG module, which
channel shall be active while switching to such a channel.
You get with the 2. Byte IdentExt in PMCT:
D0 = Check-DD 
D1 = no Check-DD
A0 = L/R (Default) 
A1 = L Audiokanal 
A2 = R Audiokanal

- Function to repeat DiSEqC command for two times
For people who use a 12V- or option-switch cascaded together with a multi-switch, there is a problem
to get the commands in correct order to the switches. With this option in Config Menu it is possible
to send the DiSEqC command two times. One time before setting the 12V voltage and a second
time after setting it, to avoid switching problems, which results in getting no signal.

- O-EPG to get ToH EPG mode
In this version the original Humax EPG is called while pressing the EPG key on the remote
control. If you want to have the ToH EPG module, you get it by pressing 0+EPG.

- Pacman
Nothing to say about. Only enjoy it :-)

=========================================
Have Fun With Our Stuff
Planet_Hemp/us/Padawan/HUMI_USER
Your ToH Team
=========================================
