Tableless version

Directories in `/pub/cbm/schematics/computers/vic20/`
The VIC-20 and the VIC-20CR
`../` | [Parent directory]
`cartridges@` | Commodore VIC-20 cartridges
`drives@` | Disk drives
`firmware@` | System firmware

Files in `/pub/cbm/schematics/computers/vic20/`
| Date | Size | Filename | Description
--- | --- | --- | --- | ---
| 1996-05-08 | 130771 | `251027l1.gif` |
| 1996-05-08 | 173902 | `251027l2.gif` |
| 1996-05-08 | 103747 | `251027l3.gif` |
| 1996-05-08 | 146612 | `251027r1.gif` |
| 1996-05-08 | 165161 | `251027r2.gif` |
| 1996-05-08 | 136724 | `251027r3.gif` | VIC-20CR rev.D (NTSC, new design). Assy number 251027-01. The PAL model has a crystal frequency of 4433618 Hz, and there is an extra 56pF capacitor on the solder side of the board, soldered parallel to R5.
| 1996-05-08 | 177837 | `324001_1.gif` |
| 1996-05-08 | 194380 | `324001_2.gif` |
| 1996-05-08 | 170958 | `324001_3.gif` | VC-20 rev.B (PAL, old design). Assy number 324001-03. Bad scanning quality.
| 1995-04-23 | 244980 | `vic20-left.tiff` |
| 1995-04-23 | 252038 | `vic20-middle.tiff` |
| 1995-04-23 | 168022 | `vic20-right.tiff` | This diagram is scanned from the Commodore VIC-20 Programmer's Reference guide. It describes an early NTSC motherboard and most probably contains some errors, like the Commodore 64 schematic from the Commodore 64 PRG does.
| 1996-05-08 | 37570 | `vic20bus.gif` | A block diagram of the VIC-20 bus signals.
| 1996-05-08 | 111269 | `vic20mod.gif` | The VIC-20 RF modulator (PAL).

[FTP://NIC.FUNET.FI/pub/cbm/schematics/computers/vic20/ | SunSITE ftp | SunSITE http]

Problems? Please consult /pub/cbm/README, /pub/cbm/README.FILETYPES and /README.FILETYPES!

Tired of downloading? See /pub/cbm/README.CD-ROM.