Table-based version

## Directory `/pub/cbm/firmware/computers/vic20/`

`../`
  [Parent directory]
`drives@`
  Disk drive firmware
`schematics@`
  VIC-20 and VIC-20CR schematic diagrams

`README`
  VIC-20 parts and firmware versions
`basic.901486-01.bin`
  Commodore VIC-20 BASIC V2. The first and only version.
`characters.901460-03.bin`
  Commodore VIC-20 character generator ROM.
`characters.NecP22101-207.bin`
  Commodore VIC-20 character generator ROM for Swedish/Finnish character set.
`kernal.901486-06.bin`
  Commodore VIC-20 KERNAL ROM, revision 6. Intended for NTSC-M systems. Probably not the first revision. But not the sixth revision either, since the BASIC ROM has the same part number.
`kernal.901486-07.bin`
  Commodore VIC-20 KERNAL ROM, revision 7. Intended for PAL-B systems. Probably the last revision.
`kernal.NecP22081-206.bin`
  Commodore VIC-20 KERNAL ROM, 901486-07 version patched for Swedish/Finnish keyboard and character set. Chip markings: NEC JAPAN P22489-207 / D2364C 689 UE12 (Yes, it is a 8kb*8 mask-programmable ROM!).
`kernal.differences`
  Lists the differences between the VIC-20 KERNAL ROMs 901486-06 and 901486-07.

[FTP://NIC.FUNET.FI/pub/cbm/firmware/computers/vic20/ | SunSITE ftp | SunSITE http]

Problems? Please consult /pub/cbm/README, /pub/cbm/README.FILETYPES and /README.FILETYPES!

Tired of downloading? See /pub/cbm/README.CD-ROM.