Calin's Humble Scanner - User Guide

## Scan method Multicast Listener Discovery

Multicast Listener Discovery is a protocol used by an IPv6 router to discover the presence of multicast listeners on its directly attached links.
See RFC 2710 and RFC 3810 for more informations.

To specify a multicast address set it as :

- if empty, All Nodes link-local
- NN for All Nodes node-local
- NL for All Nodes link-local
- RN for All Routers node-local
- RL for All Routers link-local
- RS for All Routers site-local
- user supplied IPv6 address

For this method the Operating System Mimic technology is NOT implemented yet.

[ User Guide | Scan Methods ]

Copyright © 2006 - 2009 Calin Radoni Hosted on http://www.geocities.com/calinradoni Last page modification is 27 May 2006