Checklist CRDA Cant Z.1007bis for FS2002
by Pierino Primavesi


     NORMAL PROCEDURES

___________________________________________

     Before Starting Engines

1.  Brakes: ON
2.  Battery Switch: ON
3.  Generators: OFF
4.  Pitot: OFF
5.  Navigation Lights/Strobe : AS REQUIRED
6.  Ailerons: CHECKED
7.  Rudder: CHECKED
8.  Flap Handles: NEUTRAL
9.  Trim: CHECKED THRU FULL MOVEMENT AND 
          RETURNED TO NEUTRAL
10. Doors and Hatches: CLOSED 
          (use spoilers switch)
11. Fuel Quantity: CHECKED
12. Tank Selector: BOTH
13. Mixture 1-2-3: RICH
14. Pitot: ON

___________________________________________

     Starting Engines 1-2-3

    --------------------------
1.  Magnets Engine 1: BOTH
2.  Engine 1: START
3.  Propeller 1: FORWARD (2'200 RPM)
4.  Oil Pressure 1: CHECKED
5.  Fuel Flow 1: CHECKED
6.  EGT 1: CHECKED
7.  Throttle 1: ADJUSTED
8.  Mixture 1: CHECKED
9.  Battery Switch: OFF
10. Magnet 1 R: CHECKED (MAX - 10%)
11. Magnet 1 L: CHECKED (MAX - 10%)  
12. Propeller 1: LOW (1'000 RPM)

    --------------------------
1.  Magnets Engine 2: BOTH
2.  Engine 2: START
3.  Propeller 2: FORWARD (2'200 RPM)
4.  Oil Pressure 2: CHECKED
5.  Fuel Flow 2: CHECKED
6.  EGT 2: CHECKED
7.  Throttle 2: ADJUSTED
8.  Mixture 2: CHECKED
9.  Magnet 2 R: CHECKED (MAX - 10%)
10. Magnet 2 L: CHECKED (MAX - 10%) 
11. Propeller 1: LOW (1'000 RPM)

    --------------------------
1.  Magnets Engine 3: BOTH
2.  Engine 3: START
3.  Propeller 3: FORWARD (2'200 RPM)
4.  Oil Pressure 3: CHECKED
5.  Fuel Flow 3: CHECKED
6.  EGT 2: CHECKED
7.  Throttle 2: ADJUSTED
8.  Mixture 2: CHECKED
9.  Magnet 3 R: CHECKED (MAX - 10%)
10. Magnet 3 L: CHECKED (MAX - 10%) 
11. Propeller 3: LOW (1'000 RPM)

___________________________________________

     Before Taxiing

1.  Battery Switch: OFF
2.  Generators: ON
3.  Pitot: ON
4.  Ailerons: CHECKED
5.  Rudder: CHECKED
6.  Flap Handles: NEUTRAL
7.  Trim: CHECKED THRU FULL MOVEMENT AND 
          RETURNED TO NEUTRAL
8.  Flight Controls: FREE WITH FULL TRAVEL
9.  Tank Selector: RT.MAIN, LT.MAIN, BOTH
10. Autopilot: OFF
11. Radio, Time and Altimeter: CHECKED
12. Hydraulic Pumps and Pressure: CHECKED
13. Altimeters: SET
14. Air Speed: STATIC
15. Instrument Suction: CHECKED
16. Fuel Quantity: CHECKED
17. Fuel Pressure: CHECKED
18. MAGS. and GEN: CHECKED
19. Oil Temp. and Press: NORMAL FOR TAKE-OFF
20. Care. and Cyl. Head Temp: NORMAL FOR TAKE-OFF
21. Flaps: UP
22. Brakes: OFF

___________________________________________

     Taxiing

1.  Check Turn and Bank Gyro Inst. While Taxiing
2.  Do NOT Idle Engines Below 800 RPM
3.  Check Brakes While Taxiing
4.  D.G. and Horizon: UNCAGED and SET
5.  ADF: ON, STATION IDENTIFIED AS REQUIRED
6.  Weight and Balance: CHECKED
7.  Trim Tabs: SET FOR TAKE-OFF
8.  Mixture: RICH
9.  Propellers: CHECKED AND IN TAKE-OFF POSITION
10. Flight Controls: FREE WITH FULL TRAVEL

___________________________________________

     Before Take-Off

1.  Mixture: RICH
2.  Fuel Valves: BOTH TANKS
3.  Altimeter: SET
4.  Gyro and Suction: CHECKED
5.  Pitot: ON
6.  Trim Tabs: SET FOR TAKE-OFF
7.  Flaps: AS REQUIRED
8.  MAGS. and Generators: CHECKED
9.  Flight Controls: FREE, FULL TRAVEL

___________________________________________    

     Take-Off

1.  Propellers: 2'300 RPM
2.  V1: 100 KM/H
3.  VR: 120 KM/H
4.  V2: 120 KM/H

___________________________________________

     Climb

1.  Autopilot: AS REQUIRED
2.  Navigation Lights/Strobe : AS REQUIRED
3.  Pitot: OFF / AS REQUIRED
4.  Altimeter: CHECKED
5.  Vertical Speed: CHECKED
6.  Flaps: UP / CHECKED
7.  Oil Pressure 1-2-3: CHECKED
8.  Oil Temperature 1-2-3: CHECKED
9.  Fuel Flow 1-2-3: CHECKED
10. Propellers: 2'300 RPM MAX

___________________________________________

     Cruise

1.  Autopilot: AS REQUIRED
2.  Airspeed: 350 KM/H
3.  Flaps: UP
4.  Altimeter: CHECKED
5.  Gyro: CHECKED
6.  Mixtures: AS REQUIRED

___________________________________________

     Approach and Landing

1.  Landing Weigth: CHECKED
2.  Autopilot: AS REQUIRED
3.  Oil Pressure 1-2-3: CHECKED
4.  Pitot: ON
5.  Altimeter: SET
6.  Fuel Selectors: LEFT MAIN, RIGHT MAIN 
          OR BOTH TANKS
7.  Mixtures: RICH
8.  Brakes: OFF
9.  Navigation Lights/Strobe : AS REQUIRED

___________________________________________

     Landing

1.  Autopilot: OFF
2.  Altimeter: SET
3.  ADF: AS REQUIRED
4.  Flaps: DOWN / AS REQUIRED
5.  Airspeed: 110 KM/H

___________________________________________

     After Landing

1.  Propellers: 1'300 RPM
2.  Flaps: UP
3.  Trim Tabs: Neutral
4.  Pitot Heat: OFF
5.  Propellers: MIN RPM
6.  Mixture: LOW
7.  Magnets Engines 1-2-3: ALL OFF

___________________________________________

     Secure Aircraft

1.  Park Brakes: ON
2.  Electrical Switches: ALL OFF 
3.  Battery Switch: ON 
4.  Battery Switch: OFF 
