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	Methods of rigging a jib on a Corsair varies, from boat to boat as do types of fittings used by each skipper.

This list is intended as a guide to help boat owners and is the most common method used.

Click on the hardware photo to get a bigger size.

	Jib Halyard


Jib Tension



	

RONSTAN website click on the logo above
Hull & mast jib Attachment fittings

See the Constitution & Class Rules for measurements 


The first hole of the attachment deck fitting is for the fore stay. Attach the jib tack to the 2nd hole This will enable the boat to sail close to the wind.



The jib can be attached to the jib halyard with a shackle or a shackle and a swivel barrel.  See photo top left side. Hoist jib fully by pulling the halyard.
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Jib Furler set up


To attach the jib halyard to a vang system, make sure that the jib wire passes trough the Mast D Ring. 


Jib Tension
Attach the bottom of the vang system to the mast saddle with a twisted shackle and the top to the jib halyard. The most suitable vang system for the jib tension is  4.1 See left side photo
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Jib Downhaul
Connect a single cheek pulley to the third last hole from the deck attachment fitting. Put robe through the last hole and put a figure eight knot on the end of robe. Take the length of the robe through jib clew cringle then pulley and then to a cleat next to the mast tabernacle. 
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