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	This is an information page how you could rig your Corsair Vang.

 Pulleys & cleats are a very personal preference, below is just a guideline.

	Mast Diagram


	

Boom Diagram


To attached stainless steel Boom hangers See Boom Diagram.
31. From the front of the boom to the boom vang attachment Point. 

Measurement 1'10" Ft ins, 559 mm, Tolerance + 0'2" " Ft ins, + 51mm
35. From the boom vang attachment point to the lower edge of the boom.

Measurement 0'0-3/4" Ft ins,19 mm, Tolerance + 0'0-l/4" Ft ins, + 6.5 mm

To attached stainless steel Mast hangers See Mast Diagram

25. From the attachment point of the boom vang to the extremity of the mast foot casting.

Measurement  0'8" Ft ins, 203 mm, Tolerance + 0'0" " Ft ins, +  0 mm
26. From the inside of the attachment point of the boom vang fitting on the mast to the aft edge of the mast.

Measurement 011" Ft ins, 26 mm, Tolerance + + 0" Ft ins, + 0 mm
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RF51 S Hook 


RF30110
swivel shackle head
Series 30mm


Rope to suit your choice of vang
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RF187
Fiddle, v-jam cleat, tube rivet head

Series 25mm & 29mm Narrow
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Ronston more Vang Systems 

VANG 1

Basic 3:1 Vang system suitable for use on small dinghies to 3m (10ft) in length. Incorporates integral V-Jammer cleat.
MWL = 300kg (660 lb)
Max Line Size = 6mm (1/4")


VANG 2

4:1 variation of the previous system providing a little more purchase if needed. Fiddle blocks ensure clean free running system without cross overs.
MWL = 300kg (660 lb)
Max Line Size = 6mm (1/4")



VANG 3

Compact 4:1 small dinghy vang system. Lower profile achieved through use of side-by-side double blocks and integral V-Jammer cleat.
MWL = 375kg (820 lb)
Max Line Size = 6mm (1/4")
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