[R.A.W Productions]
[01.13.92]
      
      
      [A Complete Guide To Hacking and Use of ASpEN Voice Mail Systems]
                            [Written by: Caveman]                
                              
           
[Introduction]

     ASpEN, or "Automated Speech Exchange Network," is a voice mail system
used by small businesses for individual employees' when away from their
desks. It is, in my opinion, by far the easiest system to use. There are
other vms's to hack on, but many can be difficult, including systems that 
require a "box/password" number to be entered (which any stupid shit knows 
is as difficult as a GOOD meal with spam in it; close to impossible of 
course.) 
     I will be discussing the basics and commands of the ASpEN systems, 
If you need information on voice mail systems in general, or info on another
specific type of voice mail system, I highly suggest the LoL article on 
hacking voice mail boxes, as well as the article on hacking voice mail boxes 
by Night Ranger in Phrack #34, both are good sources of information. 
     
[Finding An ASpEN System]

     In order to find an ASpEN system, you will need to get some form of 
wardialer. I've heard a lot of shit about what's the best, I don't give a 
fuck, they all do the same damn thing. The easiest way to find a voice mail
system is set up a wardialer, connect a spare phone to the second phone slot 
on your modem, and set up the wardialer to an exchange that is known to carry
voice mail systems (i.e. 1-800-666-XXXX) After a shitload of ringings, stanky
operators, and fax machine ringings, you will come across something that 
sounds like an answering machine. If you are extremely lucky, you will come
across the generic message that comes with the ASpEN system. You will hear:

        "Hello, this is ASpEN, the Automated Speech Exchange Network. Please
        enter the number of the person you are calling. If you have a mailbox
        on this system, please press pound."

Otherwise you will get a recording from the company itself, in which case you
need to press the star key to enter the voice messaging system. If you get a 
message saying, "Mailbox number please" you have found a voice mail system. It 
is not necessarily an ASpEN system, it could be one of a number of systems. In 
order to know absolutely that the system you have found is ASpEN, you will 
need to recognize the ASpEN computer voice. If you need a sample of the voice, 
call 1-800-852-MAIL and press pound (#). You will get a sample of the ASpEN 
voice from this system. After determining that you have indeed found an ASpEN 
system, you are ready to go to work. You have already done the hardest part, 
finding an ASpEN system.

[The 800 Exchange Problem] 

1-800 voice mail systems are by far the most useful, for obvious reason of low 
cost calling from around the country, so that phreaks and hackers from coast-
to-coast are able to contact you. However, there has been a problem with 
attempting to hack an 800 exchange. It is the simple fact the each time you
call the 800 system, the system itself gets billed for the call. Even if you 
are lucky enough to find a local 800 voice mail system, the system will still
be billed for the call. If you are calling a long distance 800 exchange, 
the system will be billed for the LONG DISTANCE bill. Thus, if you call the 
system many times in search of a box, then the System Administrator will be
notified of irregular patterns in the bill at the end of the month, including 
multiple long distance calls from the same source in a short period of time.
The System Administrator, if competent, will check the system for hackers,
and will eventually find your box. The risk of the System Administrator 
sighting the irregular phone bill, or practicing "Preventive Maintanence 
Excercises," all depends on the size of the system, the size of the company 
paying for its use, as well as if the system regularly receives many long
distance calls.

[3-Digit Error]

     The reason that ASpEN is the easiest is some "errors" in the programming 
of the automated system. Among the most useful is the 3-digit error. If you 
enter three numbers SLOWLY, such as 1-5-2, taking your time with each number 
you enter, then at the end of the THIRD number, the ASpEN computer-generated 
voice will tell you: 

        "Box 1-5-2 is not a recognized mailbox, please try again. Please re-
        enter your mailbox number."

By not allowing the user to enter the fourth number, the ASpEN system has, in
effect, told you that there are NO mailboxes in the 152 exchange, in other 
words, no 1520, 1521, 1522, 1523, etc... up to 1529. Instead of having to 
check all ten of these boxes, you only need enter the first three numbers 
slowly and wait for the system to tell you that they are invalid. If the 
1-5-2 exchange is invalid, then try the next exchange, 1-5-3. However, if
you enter 1-5-2 and the system pauses and waits for another number, then 
BINGO, orgasm, you have found a valid exchange, meaning that there is a valid 
mailbox between 1520 and 1529. In the pause between the 1-5-2 you entered and 
the computer voice not coming on, you then enter another number between 1-9.
If you get the invalid box voice again, try another number between 1-9, if
the system paused with this exchange, there is definately a box there. It may 
take you a while to find an exchange that the system will pause on, but I 
suggest looking in the range of 2400-6000, this is where I personally had the 
most success. Once you have found a mailbox, don't spooge in your pants yet,
you must begin the next step, finding a box not in use.

[Finding YOUR Box]

First, I will stress NEVER FUCKING TAKE A BOX THAT IS ALREADY IN USE BY 
SOMEONE. I can tell you, all that this accomplishs is that you get a VMB and 
you feel good for a couple of days, but as soon as the owner checks their box, 
but finds that some little shit took it over, they will report directly to 
the System Administrator, who will make a complete system check, and destroy 
any other box that WASN'T origionally in use, that some hacker obtained 
through hard work. By finding a box that isn't already in use, you are 
insuring that other hackers on the system will not be caught, as well as 
guaranteeing the safety of your own box. So how DO you find a box not in use 
on an ASpEN system? Any box that is not in use is NOT going to have a recorded 
name (a feature discussed later in the text.) While trying to find a box in 
the 3-digit method described above, you will enter a box number and come up 
with the normal ASpEN voice stating the following:

        "Hello. This system can enable you to receive messages while you are
        away from your desk... [After a lot more shit, the voice will say]
        Your System Administrator has assigned you a temporary password. 
        Please enter that password now."

When you have come upon this generic message, you have found an activated 
mailbox that is not in use, but rather reserved for a future user of the 
system. NOW HOW CAN I PUT THIS KNOWLEDGE TO WORK FOR ME? At this time, you 
begin to try the defaults for the ASpEN systems as named in Night Ranger's 
article in Phrack #34. The defaults that I have had the most success with is 
1111, the box number itself, and 1234. But before you give up, expend ALL of 
the defaults. 

[Once In The Box]

Once you have entered the correct default password for the box that of course
was NOT IN USE, the computer voice will say:
        
        "Thank you. You should now change the default password. Make it a 
        number that will be easy for you to remember but hard for others to 
        guess..."

At this point, the ASpEN will also ask you to change your recorded name and
recorded message (discussed later, and I'm sure, really difficult to figure
out.) Now, you have complete control of the mailbox. Once you have a mailbox,
post the number on your local board, so that others may share in your joy, 
and posting the default is helpful as well as the number range of the boxes.

[Commands]

When in your box, there will be a number of commands available to you. Once 
you are in your mailbox, the mailbox will tell you "No messages. Send, press
two, check receipts press three.) The option that it does not tell you on
some systems (the most important option) is "Personal Options," which menu you 
can enter by pressing 4 on your numeric telephone pad. The following is an 
outline of the options available from each menu that can be entered on the 
ASpEN system (all quoted options are taken from the "rapid prompts;" which is
what I suggest you set your prompt level to when taking over the box):

[MAIN MENU]

"Send, press 2" - to send a message from YOUR mailbox to a fellow hacker on 
                  the system. It will record your message, then ask which 
                  box to send the message to. You can enter multiple box 
                  numbers, which serves as a multi-mail service.

"Check receipts, press 3" - Once you have sent a message, and want to check
                  whether the person has received the message, or if the 
                  message you have sent is still in their mailbox, you use 
                  this option. It will ask which box to check, once you have
                  entered this, it will play their recorded name, and say 
                  either "One message from you in that mailbox" and play the
                  message over to you, or say "All messages have been 
                  received."

"Personal options, press 4" - This is basically command central of your box,
                  a number of options are contained (see PERSONAL OPTIONS
                  SUBMENU)

"Restart, press 5" - This will bring you to the origional logon message of 
                  your particular voice messaging system.

"Disconnect, press *" - If you cannot figure this out, you do not need a box.


[PERSONAL OPTIONS SUBMENU]

"Notification on or off, press 1" - This is an option that you NEVER WANT TO
                  ACTIVATE. This is an option that will call your house 
                  whenever you receive an "urgent" message. Of course, if you
                  activate this, and give your home phone number, then if the
                  System Administrator is not a shit-for-brains (as many of 
                  them are) they will be able to contact you at your home and
                  cause you more trouble than this option is worth.

"Administrative options, press 2" - This is another submenu (see
                  ADMINISTRATIVE OPTIONS SUBMENU) that contains the 
                  maintanence options.

"Greetings, press 3" - This contains another submenu full of options for your
                  greetings. (see GREETINGS SUBMENU)

"Notification schedule" - This is the option to set the time that the system
                  should call your house with "urgent" messages. As I said 
                  before, you've got to be fucked up to activiate this, it's
                  a deathwish.


[ADMINISTRATIVE OPTIONS SUBMENU]

"Passwords, press 1" - Simply the passwords of your system. (see PASSWORDS 
                  SUBMENU)

"Prompt level, press 3" - The level of explanation the ASpEN system gives 
                  you when reciting your options. Prompt level 1 is set for 
                  morons, level 2 is for a user just getting used to the 
                  commands of the ASpEN system, and level 3 is rapid prompts,
                  the briefest ASpEN messages the system allows.

"Date and time options, press 4" - This allows you to enable or disable the
                  date and time option, which stamps each incoming message
                  with the date and time of receipt.

"To exit, press *" - Whenever you are in a submenu, and want to exit to the 
                  menu you were in prior to the submenu, press the star key.
                  You will be transfered to the previous menu, or if you are
                  in the main menu, you will disconnect.


[GREETINGS SUBMENU]

"Personal greeting, press 1" - Your personal greeting is what the caller will
                  hear when calling your box.

"Extended absence greeting, press 2" - This is used by companies when their
                  employees take vacations, and there is no need for them to 
                  receive messages. With this option on, you will not be able 
                  to receive messages until the extended absence greeting is 
                  deleted. This is useful when you are switching mailboxes,
                  and want to convey to the caller your new system and box 
                  number, and make it impossible for the caller to leave a 
                  message.

"R

