

                   ***************************************
                   *                                     *
                   *        The 1986 COSMOS FILES        *
                   *    PART III: Service Order Input    *
                   *             Written by:             *
                   *                                     *
                   *            SIR WILLIAM              *
                   *              [KOTRT]                *
                   *                                     *
                   ***************************************



The 1986 COSMOS FILE series consists of 6 parts, including the introduction,
covering all major Service Orders, Work Orders, Reports, Facility and Circuit
Alteration, COSMOS-N/PREMIS transactions and a complete list of all the
facility prefixes.  The 1986 file series is intended for the serious COSMOS
hacker.  (Not too serious)

NOTE: The content of this material is proprietary and constitutes a trade
secret.  It is furnished pursuant to written agreements or instructions
limiting the extent of its disclosure.  Its further disclosure in any form
without the permission of its owner, Western Electric Co. Inc., is prohibited.
hi ho.

DISCLAIMER: I take full responsibility for all deaths, physical injuries,
            emotional stress, and monetary damages as a result of this file.
            Please send all claims to KOTRT Enterprises, P.O. Box 1223-232,
            Wunderland, N. Ireland 928301

                   ***************************************
                        INTRO TO SERVICE ORDER INPUT
                   ***************************************

Under COSMOS software version 8.X there are new input procedures for SOE's.
Although these are mostly in the area of error handling, they require a bit
of discussion, seperate from the basic input.

    Error Handling
    --------------
      Service order transactions interact with the user more frequently in
      REV 8.X.  Each time the transaction is ready for a new input, it will
      respond with and underscore "_" at the beginning of the new line.  This
      indicates that the preceding line is correct.
      If an error does occur, the transaction will respond with an error
      message and prompt for correction.  When an error occurs, you have
      4 choices.
      1.  Re-enter the entire field correctly.
      2.  Enter line-feed to ignore, (checks rest of line)
      3.  Enter a ";" to disregard the present circuit.
      4.  Enter a "." the transaction will disregard all input, and exit.
 
   H-LINE inputs.
   --------------
      H-LINE input for the service order trio SOE/CSA/TSA is being rigidly
defined in 8.0 according to three categories.  These categorys contain
fundamentally different types of order/facility information.
     Category 1: ORD, OT, DD, FDD,J OC, DT, SG, EO, LC
     Category 2: US, FEA, CCF, CAT, BTN, SS, AO, RZ, FR, GP/CG, CTX/CG/MG/NNX,
                 LDN, RTI.
     Category 3: FW, RW
     Category 1 items are primary, once defined they cannot be changed
                by conflicting category 2, and 3 lines.

                         SERVICE ORDER TRANSACTIONS

   Transaction         Definition
   ===========      ======================
   SOE              Service Order Input
   TDZ              Telephone Number Assignment lists
   LDZ              Line Equipment Assignment list
   SOH              Service Order withheld
   SOM              Service Order Modification
   SOC              Service Order Cancellation
   SOW              Service Order Withdraw
   SCM              Service Order Completion by MDF
   SCP              Service Order Completion by PAO
   SCA              Service Order Completion - Automatic
   SCF              Service Order Completion for MDF automatic
   SCI              Spare Cable pair inquiry
   CDD              Change Due Date
   BAI              Bridge Lifter Assignment Inquiry
   LAI              Line Equipment Assignment Inquiry
   NAI              Telephone Numbers Assignment Inquiry
   TAI              Tie pair assignment Inquiry
   EDZ              Facility Emergency Assignment list for backup
   MAP              Manual Assignment Parameters
   MAL              Manual Assignment list
   TSW              Total Service Order Withdraw

                   ***************************************
                           TRANSACTIONS DEFINED
                   ***************************************

SOE - Service Order Establishment
    - Establishes a pending service order.  The types of orders are; NC, CD,
      CH, F, T, SS, RS, R, RF.  Reassociations are treated as change orders.
    - H-lines must contain ORD, DD, and OT.  Optional facilities; FW, RW, FDD
      AO, FR, SG, and either DT or OC.
    - I and O lines may contain; US, FEA, CP, OE, TN, RZ, NNX, PL, TP, TK, BL, #     SE, CON, MR, BTN, RC, RE, RT,STC, STN, STO, CCF, LCC, and RTI.
    - ESS orders requiring coordination by the recent change input center may  #    be flagged with an input of "RW C".
Example of a NC [New Connect]
WC% SOE
H ORD NCXXXXXX/DD 01-01-86/OT NC/FDD 02-05-86/DT AM
_I CP XXXXX-XXXXXX/OE ?/TN ?/US 2FR/FEA RNNL
_.

Example of a CD [Complete Disconnect]
WC% SOE
H ORD CDXXXXXX/DD 01-01-85/OT CD
_O TN 534-1822
_.

Example of a CH [Change]
WC% SOE
H ORD CHXXXXX/OT CH/DD 01-01-86/TN 534-1822
_O TN 534-1822/STN CO
_I TN ?
_.
Example of SS [Suspension]
WC% SOE
H ORD SSXXXXX/OT SS/DD 01-01-86
_O TN 534-1822/SS SB
_.

TDZ - Telephone Number Assignments List
    - List the indicated number of spare directory numbers for a NNX code, and
      directory number type.
    - Up to 25 directory numbers can be specified, using the prefix LC.
Example
WC% TDZ
H NNX 534/TT G/LC 7    (LC can be up to 25)
.
Output example would look similar to this.
**EMERGENCY FACILITY ASSIGNMENT LIST 01-01-86
  RESERVED LINE EQUIPMENT
**NO SPARE LINE EQUIPMENT FOUND
  AVAILABLE DIRECTORY NUMBERS (7)
534-XXXX
534-XXXX, etc.
**TRANSACTION COMPLETED

SOW - Service Order Withdraw
    - Withdraws most recent version of a service order
    - Order number must refer to the latest version.  The H-line circuit ID
      identifys the order.  Valid circuit identifiers are; TN, XN, PL, CP, OE,
      and TK.
Example
WC% SOW
H ORD NC-XXXXX/TN 534-1822
.

SCP - Service Order Completion by PAO
    - Record in the Service Order File the completion of an order by PAO
    - Standard SXX H line input.
Example
WC% H ord CDXXXXXX/TN 534-1822
.

SCA - Service Order Completion Automatic
    - Enters final completion on all service orders which have been or are
      not requried to be completed by the MDF, are not in a held, or jeopardy
      status, and are due prior to or on the current date.
    - Two due dates may be entered on the H-line; SCA will complete orders due #     on or between the dates.  Additional options are OT (order type), ORD,
      and SG.
Example
WC% SCA
.          :complete all orders on or before this due date

Example2
WC%SCA
H DD 01-01-86/OT NC     :Complete all NC (new connect) orders
.


CDD - Change Due Date
    - Change due date of a service or frame order
    - I think an example will suffice;
WC% CDD
H ORD CH-XXXXXX/TN 534-1822
I DD 01-01-86
.
output example
**ORD CH-XXXXX  DUE DATE 01-01-86


NAI - Telephone Number Assignment Inquiry
    - Provides from 1 to 25 spare telephone numbers compatable with the
      input specifications.
    - Input is an H-line with the TN type and NNX or RZ entries. The status of
      the TN supplied will be modified to reserved if ST is specified on the H-#     line.
Example
WC% NAI
H TT X/NNX 534/ST RS
.
this shows first available spare in prefix 534.

MAP - Manual Assignment Parameter
    - Permits the PAO to establish the parameters that will constitute the PAO #     Open-of-Day report.
WC% MAP
I NNX 534/ECS 1R/EQF TNNL/LC 50, etc.   (for line equipment)
I NNX 534/TT B/LC 10  (For Telephone numbers of type B, 10)
etc.

    ==============================================================
     [C]OPYRIGHT 1986.  KOTRT ENTERPRISES.  WUNDERLAND, S. AFRICA
    ==============================================================


Downloaded from P-80 Systems.....

                           