All Siemens Phones: Service Provider Unlock: *#0003*(secret code 8 digits)#

Siemens S25/C25

SP unlock *#0003*(secret code 8 digits)#
Show IMEI code: * # 06 #
Resets language to automatic selection : * # 0000 # then Green button
Pin Out
Data Cable schematics
Phone's connector pin-out:
1- GND
2- SB
3- POWER
4- NC
5- TX
6- RX
7- CLOCK
8- DATA
9- GND MIC
10- HF MIC
11- AUDIO
12- GND AUDIO

Siemens S1/S3/S3 Com

To view the software date and else with S3 com, S4, S4Power, Sony cmdx 1000e press with SIM removed *#06# and left softkey.
To view some other stuff with S4Power, Sony cmdx 1000e press with SIM removed *#06# and left softkey twice.
To view the software date with S3 com, S4, S4Power, Sony cmdx 1000e press with SIM installed menu 98 and left softkey twice.
ACTIVATE MONITOR MODE
Siemens S1/S3

Menu, 9 (Phone Options), 7 (Phone Status), Left Display Button (left MENU key), 5553756, Hang-Up Button (Red Handset key)

Siemens S3 COM/S4

Menu, 9 (Phone Options), 7 (Phone Status - 8 on Some), Left Display Button (left MENU key), 7684666, Hang-Up Button (Red Handset key)

Note: Now Monitor should appear at the bottom of the Network Options menu.
MONITOR MODE
Pressing the right Display Button when in monitor mode will toggle into 1 and 2 modes

Pressing the right Display Button when in monitor mode will show a list of the six cells with the strongest signals.

Test Mode Indicators: (* = only available when call in progress )
CH Channel Number

RX Signal Strength (dB)

N NCC (Colour Code)

B BCC (Colour Code)

CI Cell ID (in Hex)

C1+ How long before phone does forced hand over. (see RX and RXAM)

LAI Location Area Identity. Display Network ID code (42F010 = 240.01) and MSC

TXPWR Transmit Power (dB)

RXAM Receive signal strength cut-off point

TS* Time Slot Number

TA* Timing Advance. Distance from tower in Km X 2

PL* Power Level
POWER table
PL: 5 6 7 8 9 10 11 12 13 14 15

dB: 33 31 29 27 25 23 21 19 17 15 13

Watts: 2 1.3 .8 .5 .3 .2 .13 .08 .05 .03 .02
LF* C1 value with continuous transmission from tower

LS* C1 Value with discontinuous transmission from tower

QF* Bit Error Rate with continuous transmission from tower

QS* Bit Error Rate with discontinuous transmission from tower
BER (bit error rate) table
QF/QS register: 0 1 2 3 4 5 6 7

% of bit sent: 0.2 0.8 0.4 1.6 3.2 6.4 12.8 25.6

Siemens S1/S3

Here's a trick to play Tetris, also known as Klotz on a Siemens S1.
Turn the phone on. Enter PIN. Before the telephone has logged in to the your GSM net do the following steps.
1: Choose F 9 (function settings)
2: Choose send own number and push the right button for choose.
3: Push 9
USE 2 as < and 8 as > , rotate the klotz with 5 and drop with 4.
[I have just heard from one of the programmers of the phone that Tetris was in the phone during development, but it was removed before it was produced. Apparently someone has the patent on games in mobile phones and Siemens didn't want to pay the licensing fees. It was either in Menu F-9-9 or it's not there at all.]

Siemens S3 Comfort

MONITOR MODE

The Siemens S3 Com series have a Monitor mode that can be activated directly from the standard user keypad. In order to activate this mode, you must enter the special access code currently programmed into the phone.
TO ACTIVATE MONITOR MODE:
Turn the phone on.
Enter the PIN access code on press OK. (Only if is enabled).
Press Menu. (Left top button).
Press 9. (Phone Options).
Press 8. (Phone Status) (May be button 7 in some phones).
You may see your IMEI Number
Left Display Button (Top left MENU key).
7684666
Hang-Up Button. (Red Handset key).

Note: Monitor should appear now at the bottom of the Network Options menu.
MONITOR MODE

Pressing the right Display Button when in monitor mode will toggle into 1 and 2 modes

Siemens S4/S4 Power


In phonebook under "Own Phone No." enter +12022243121 (which is the number to the White House) and you'll get a greeting from the people who programmed the phone.

MONITOR MODE

The Siemens S4 series have a Monitor mode that can be activated directly from the standard user keypad. In order to activate this mode, you must enter the special access code currently programmed into the phone.
TO ACTIVATE MONITOR MODE:
Menu, 9 (Phone Options), 7 (Phone Status), Left Display Button (left MENU key), 7684666, Hang-Up Button (Red Handset key)
Now "Monitor" should appear at the bottom of the Network Options menu.
Pressing the right Display Button when in monitor mode will show a list of the six cells with the strongest signals.


Test Mode Indicators: (* = only available when call in progress )

--------------------
CH Channel Number

RX Signal Strength (dB)
N NCC (Color Code)
B BCC (Color Code)
CI Cell ID (in Hex)
C1+ how long before phone does forced hand over. (see RX and RXAM)
LAI Location Area Identity. Display Network ID code (42F010 = 240.01) and MSC
TXPWR Transmit Power (dB)
RXAM Reeceive signal strength cut-off point
TS* Time Slot Number
TA* Timing Advance. Distance from tower in Km X 2
PL* Power Level


Power Table

PL: 5 6 7 8 9 10 11 12 13 14 15
dB: 33 31 29 27 25 23 21 19 17 15 13
Watts: 2 1.3 .8 .5 .3 .2 .13 .08 .05 .03 .02

LF* C1 value with continuous transmission from tower
LS* C1 Value with discontinuous transmission from tower
QF* Bit Error Rate with continuous transmission from tower
QS* Bit Error Rate with discontinuous transmission from tower


BER (bit error rate) table
QF/QS register: 0 1 2 3 4 5 6 7
% of bit sent: 0.2 0.8 0.4 1.6 3.2 6.4 12.8 25.6

Siemens S6/S10

In Phonebook, store as your own number: +12022243121
Then you get the sun and two palms in the display, also a greeting message of the "MMI-team".
It has been said that the phone number is the number of the Capitol building in Washington, DC (but not sure).

Siemens S15 Secret Menu's

Press * -> # -> 7 -> 4 -> 3 -> 6 -> 3 -> 6 -> 7 -> * -> 8 -> 3 ->
7 -> 8 -> # ,press clear key to clear screen and return to
stand-by mode
press Menu, it will show additional menu
Menu 3.3.4 Band selection,
Menu 3.3.4.1 Automatic band selection,
Menu 3.3.4.2 select GSM 900 only,
Menu 3.3.4.3 select GSM 1800 only,

Menu 10 Engineering,
Menu 10.1 MS info,

Menu 10.2 software detail,
Menu 10.2.1 software version,
Menu 10.2.2 EEPROM version,

Menu 10.3 Test/production details
Menu 10.3.1 Hardware deta
Menu 10.3.2 production deta
Menu 10.3.3 Service deta
Menu 10.3.4 Mechanical deta

Menu 10.1.1 MS info on, then on the screen show these, for example:

FCN RXL C1 C2
642 011+11+91 -> PAGE 1

CID DSC CB
11211 045 000 -> PAGE 2

BCC NCC TN
000 002 00 -> PAGE 3

RXf RXs RQf RQs
00 00 00 00 -> PAGE 4

ATa APa Hn Hf
001 000 05 00 -> PAGE 5

DTU DTD HP CI
+ ? - - -> PAGE 6

MM CC RR
IdNS Nul Idl -> PAGE 7
