Please unzip the attached EE file and copy both EE.exe and EE to the floppy disk.


Step 1. Check your correct MAC address: Find a bar-code sticker on the motherboard which has MAC address on it.
For example: 000B6A112233.



Step 2. Fill in the MAC address: Open EE with notepad and you will find 
0b00    ; Mac addr [2][1]
126a    ; Mac addr [4][3]
5634    ; Mac addr [6][5]

Replace them with your MAC address. Click "save" before closing the EE file.
For example: 000b6a67890a
0b00    ; Mac addr [2][1]
676a    ; Mac addr [4][3]
0a89    ; Mac addr [6][5]

**Please be careful with the right order and make sure not to change other registers.



Step 3. Prepare a boot disk which allows you to boot into DOS mode.



Step 4. Boot your system in DOS mode with the boot disk. When you see A:\>, put in the EE utility disk and type 

A:\>EE EE then press "enter".  
