SPECIFICATIONS FOR BUILDINGS, WHICH MAY BE ERECTED BY TENANTS ON INDIVIDUAL ALLOTMENTS AFTER APRIL 1ST 1997

GLASSHOUSES

May only be constructed of aluminium, softwood or hardwood and to a traditional design with maximum dimensions of;

Length
3.0m (approx. 9 feet 9 inches)

Width

2.4m (approx 8 feet)

Height
2.0m (approx 6ft 6 inches) to eaves and 3.0m (approx. 9 feet 9 inches) to ridge.  All height measurements are from ground level.

Roof

Must be ridged along the entire length of the building

Covering
From ground level up to a height of 700mm (2 feet 6 inches) may be timber, aluminium sheet, Perspex or glass.  Above this height may be glass, Perspex or clear rigid polythene.

NB. No glasshouse may be constructed of waste materials such as old window frames/glazed

doors/wooden pallets etc. which have been fixed together.

SHEDS

May only be constructed of soft or hardwood timber (either close boarded, ship lapped, or

 tongue and groove), and to a traditional design with maximum dimensions of:

Length
3.0m (approx. 9 feet 9 inches)

Width

2.4m (approx 8 feet)

Height
2.0m (approx 6ft 6 inches) to eaves and 3.0m (approx. 9 feet 9 inches) to ridge.  All height measurements are from ground level.

Roof
Must be ridged along the entire length of the building or pent roofed.

Covering
From ground level up to a height of 700mm (2 feet 6 inches) may be timber, aluminium sheet, Perspex or glass.  Above this height may be glass, Perspex or clear rigid polythene.

NB. No shed may be constructed of waste materials such as old window frames/glazed 

doors/wooden pallets etc. which have been fixed together.

The positioning of any building will be within the prescribed area as determined on the site

plan which may be inspected by: a) contacting your Site Secretary




  b) Parks and Countryside Development 

      PO Box 114, Bridgewater House



      Manchester Road, Carrington M31 4WS

NOTE

1. Written request must be given to the Committee before any greenhouse, shed, polytunnel etc. is erected.

2. No more than 1 shed and or 1 glasshouse may be erected on any whole or half plot.

3. Buildings currently erected on individual allotments may be exempt from these regulations (providing that they are deigned by Council Officers to be safe), until such time as the tenancy of such allotments changes, thereafter, any buildings must comply with the above.

Written Request Form to erect any greenhouse, shed, polytunnel etc.

Full Name…………………………………………………………………..

Address……………………………………………………………………..

       …………………………………………………………………..

         …………………………………………………………………..

Allotment site………………………………………………………………..

Plot Number…………………………………………………………………

Size of greenhouse/shed/polytunnel

………………………………………………………………………………...

Signature of Consent ………………………………………………(Secretary)

Signature of Tenant…………………………………………………

Authorisation from TMBC………………………………………………………….
