KEYLESS REMOTE ENTRY

I sourced my parts from Specialized German Recycling (alarm module) and Ebay (remotes).  I have recently found that Virtual Parts World can get this as well.  I'm not sure why this surprised me though, as the Potters can get anything. You may also want to check the inventory at Impex Foreing Auto.

There seems to be a lot of trouble in selecting the correct part.  Here are a list of valid part numbers for a direct swap:

	
	1HM 937 045 M (this is the one that I installed)
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	1HM 937 045 Q (reported to work just fine)
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	1HM 937 043 B (reported to work just fine)


This will most likely not be at your local dealer.  You will have to find it at a salvage yard.  From everything I have seen, the module with keyless is white, while the plain alarm module is black.  An easy check would be the presence of an FCC ID.  This ID is given to ALL radio transmitters and receivers.  The lack of a radio means the lack of remote anything.

### YOUR FCC IDs FOR THE MODULE AND FOB MUST BE MATCHED!! ###
### THE CORRECT FCC ID IS M3GHU01Wx (where the x is either a T or an R) ###
The unit you will be looking for is manufactured by Clarion and should have an FCC ID very similar, if not identical to the ones I used.  There is a Hella module that is the same in appearance (i.e. the remotes look like keys/banjos).  It was used in New Beetles and early B5 Passats.  THE HELLA (FCC ID NBG730956x) UNIT WILL NOT WORK.
Trunk Release Instructions
Remote trunk release is not a plug and play function.  To get this functionality, Dave Schwartz has created a seperate how-to, which he has let me host here. 

Required Materials:
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	A3 Jetta or Golf with power locks (I'm pretty sure that all A3s had this, so it shouldn't be a problem)
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	OEM Volkswagen Alarm module from a 98+ A3 Jetta/Golf/GTI (VW part number: 1HM 937 045 M, 1HM 937 045 Q or 1HM 937 043 B )
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	Key fob with an FCC ID (mine is M3GHU01WT) matching that of the alarm module
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	10mm socket
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	Flat head screwdriver
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	Phillips screwdriver


Steps:

1. Take out the cover to the left of the headlight switch and headlight switch itself, disconnect both. 
It might be easiest to pop the airbag panel, then pop and disconnect the headlight switch, then disconnect the airbag light.  Either way both need to be removed, so however you find it easiest. 
2. Push aside the cords for the headlight switch and dead panel lights and you will see a little black box (the one in the picture is white because I took these pictures after the swap)
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3. Okay.. now.. under your dash, there is a big cover to protect your underside.... unscrew the 5 screws and take it off.  I also suggest that you remove the 2 screws that hold up the fuse panel cover.  I could get my whole arm up under the dash that way.
[note from golfSPORT95: this is a good time to pull the  yellow wire going to the back of relay 173 on 96 up or remove relay 94 on 93-95 A3 us models to disable Daytime running lights]  
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4. Reach up behind the alarm module and unplug the harnesses that go into it.  This is a bit easier when it is still bolted down.  The alarm module has 2 harnesses, the cruise (if you have it) has only 1. 
5. The bracket that holds the alarm module to the dash is secured with a 10mm bolt.  You will need to remove it.
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6. After taking off the bolt, manipulate the module and bracket out of the opening by the fuse panel cover.  If you took it off, this makes perfect sense because your arm is still up there from unhooking the harnesses. 
7. Unscrew the module from the bracket and switch it with the new module.  You will hear your central locking vacuums working when you plug everything back in 
8. This was a good time for me to test it all out, so you may want to skip ahead to the "Programming your remotes" section.   Don't forget to remove the spare key from the ignition when you test.  I was really confused as to why the lock wouldn't work. 
9. If everything is peachy, reverse these instructions to put your baby back together. 
Programming your remotes:
1. Put your spare key in the ignition and put it on the ON position.  DO NOT START THE CAR! 

2. Close the drivers side door (and all other doors, hood and trunk), put in the key and turn it to the left (unlock position) and hold it. 

3. The car will beep 3 times.  Let go of the key so it sits in the lock 

4. With each of the new remotes, separately, press the unlock button.  Each button will cause a "HONK" 

5. Turn the key to the left again until it beeps. 

6. Remove your spare key from the ignition. 

7. DONE! 

I have also been informed that the car may not honk at you during step 3.  

If it doesn't, all hope may not be lost.  Try to program the remotes anyway.  This was done successfully despite feedback from the alarm module. -- Thanks Brian

 

    
