The Sperry-Pilot 2.0 for FS98

These gauges simulate the Sperry-Pilot, a simple autopilot of the late 1930's.

This file replaces the older version 'Sperry.zip'. In this version the regulator 
settings are updated immediately to the Sperry-Pilot. Two new gauges are included:
- A new servo-speed-panel without an oil pressure gauge especially made for DC3's.
- An autopilot mainswitch with a 'mechanic look'

Installation:
 - Unzip the files 'SPERRY.PILOT.GAU', 'SPERRY.PILOT.SERVO.SPEED.GAU', 
   'SPERRY.PILOT.SERVO.SPEED2.GAU', 'SPERRY.PILOT.AP.SWITCH.GAU', 'SPERRY.PILOT.HLP' 
   and 'SPERRY.PILOT.CNT' to the 'gauges'-subfolder of FS98
 - Include the gauges in your panel the usual way. You should not use more than 
   one servo.speed-gauge in one panel.cfg-file.
If you have installed the previous version of the Sperry-Pilot, override the old
files and delete the 'SPERRY.PILOT.cfg' from your 'gauges' folder.


See included help file 'SPERRY.PILOT.HLP' for details.

This software package is FREEWARE. Noncommmercial use and sharing of the complete and 
unchanged package is allowed without restrictions. Including on CD's and upload to 
internet-sites wo charge fees is only allowed with explicit written agreement of the author.
This software has been tested extensivly. There should occur no problems with 3D-cards 
and force feedback devices.
Use this software at your own risk.

I like to thank Thomas Ferber for intensive test work.
I hope my English is understandable. 

Questions, suggestions, critics to
	bartels@aku.physik.uni-oldenburg.de


Bad Zwischenahn
Germany
8/27/98
Arne Bartels

