PA-28-140   Data Sheet

N7360J


1968

Serial # 28-24712

Important Airspeeds

VSO 
Stall speed, flaps down

55 mph

VS1
Stall speed, flaps up

64 mph

VR
Rotation speed


65 mph
VX
Best angle of climb

74 mph

VY
Best rate of climb

85 mph

VFE
Flap extension speed

115 mph

VA
Maneuvering speed

126 mph
VNO
Smooth Air speed

137 mph

VNE
Never Exceed speed

168 mph


Best Glide Speed

85 mph


Max crosswind


20 mph


Enroute climb speed

100 mph
Weights, Sizes, and Capacities
Oil 
capacity 8 quarts, minimum safe is 2 quarts

Fuel 
capacity 50 gallons total, 25 gallons a side, 47 gallons useable

36 gallons to tabs, 18 gallons a side
80/87 minimum octane

Engine

Lycoming O-320-E2A

150 hp. at 2700 RPM

140 hp. at 2450 RPM

Holds 8 quarts of oil

Minimum of 2 quarts of oil

Propeller
 M74DM Sensenich 74 in. dia.

58 inch pitch

Electrical

12 volt battery

12 volt 60 amp alternator

Weights

2150 lbs. max

1274.3 lbs. empty

875.7 lbs. useful load

Dimensions

Length: 23 feet 4 inches 

Wingspan: 30 feet

Height: 7 feet 4 inches

Gear Tread: 10 feet  

6.00 x 6 four ply tires 24 psi

Other Specifications

Service Ceiling 14,300 ft.
Absolute ceiling 16,800 ft.
