2.1 Clock generator - oscillator Oscillator circuit is used for providing a microcontroller with a clock. Clock is needed so that microcontroller could execute a program or program instructions. Types of oscillators PIC16F84 can work with four different configurations of an oscillator. Since configurations with crystal oscillator and resistor-condenser (RC) are the ones that are used most frequently, these are the only ones we will mention here. Microcontroller type with a crystal oscillator has in its designation XT, and a microcontroller with resistor-condenser pair has a designation RC. This is important because you need to mention the type of oscillator when buying a microcontroller. XT Oscillator
Crystal oscillator is kept in metal housing with two pins where you have written down the frequency at which crystal oscillates. One ceramic condenser of 30pF whose other end is connected to the mass needs to be connected with each pin. Oscillator and condensers can be packed in joint housing with three pins. Such element is called ceramic resonator and is represented in charts like the one below. Center pins of the element is the mass, while end pins are connected with OSC1 and OSC2 pins on the microcontroller. When designing a device, the rule is to place an oscillator nearer a microcontroller, so as to avoid any interference on lines on which microcontroller is receiving a clock. |
Connecting the quartz oscillator to give clock to a microcontroller
Connecting a resonator onto a microcontroller
RC Oscillator In applications where great time precision is not necessary, RC oscillator offers additional savings during purchase. Resonant frequency of RC oscillator depends on supply voltage rate, resistance R, capacity C and working temperature. It should be mentioned here that resonant frequency is also influenced by normal variations in process parameters, by tolerance of external R and C components, etc. Above diagram shows how RC oscillator is connected with PIC16F84. With value of resistor R being below 2.2k, oscillator can become unstable, or it can even stop the oscillation. With very high value of R (eg. 1M) oscillator becomes very sensitive to noise and humidity. It is recommended that value of resistor R should be between 3 and 100k. Even though oscillator will work without an external condenser (C=0pF), condenser above 20pF should still be used for noise and stability. No matter which oscillator is being used, in order to get a clock that microcontroller works upon, a clock of the oscillator must be divided by 4. Oscillator clock divided by 4 can also be obtained on OSC2/CLKOUT pin, and can be used for testing or synchronizing other logical circuits. Relationship between a clock and a number of instruction cycles Following a supply, oscillator starts oscillating. Oscillation at first has an uneven period and amplitude, but after some period of time it becomes stabilized. Signal of an oscillator clock after receiving the supply on the microcontroller To prevent such inaccurate clock from influencing microcontroller's performance, we need to keep the microcontroller in reset state during stabilization of oscillator's clock. Above diagram shows a typical shape of a signal which microcontroller gets from the quartz oscillator following a supply.