Run install.bat or follow the manual installation instructions below.

Manual installation instructions
-----------------------------------------
1. Copy the DOSDRV folder to your c:\ drive
2. Copy the provided autoexec.bat file to your c:\ drive or edit your current one.
3. Copy the provided config.sys file to your c:\ drive or edit your current one.
4. If you have any problems getting your setup to work make sure your card is supported and view the important notes below.

The SBLive.zip archive contains the dos sound card drivers for the Sound Blaster Live! and Sound Blaster Audigy pci cards. The are setup and optimized for MAME, however, they will not work with ArcadeOS.

Important Notes:
1. Your sound blaster pci card can not use irq 5.
2. Your sound blaster pci card should not use the same irq as your video card.
3. You must first uninstall your current sound blaster dos drivers in windows for the SBLive! drivers to work (Start/Settings/Control Panel/Add Remove Programs/Your Sound Card).
4. You can customize the irq and dma settings using the sbeset utility. For help with the sbeset.exe command line parameters in dos mode at the command prompt enter: sbeset.exe -?