REVCON Engineered Elegance 
GENERAL INFORMATION (Continued)
-- "'"
SUSPENSION SYSTEM:
~
STEERING:
ENGINE:
DIESEL ENGINE:
TRANSMISSION:
" ~
~
TRANSFER CASE:
FINAL DRIVE:
Note:
FUEL TANK:
RADIATOR:
ELECTRICAL SYSTEM:
.>

.~
BATTERY:
Rear Suspension: Free rolling tandem axles. Walking Beam with Hendrickson suspension and heavy-duty shocks.
Heavy-duty integral powerassisted steering gear, through a bellcrank and idler arm via tie rods, to wheel ends. Tilt wheel on column.
GM Chevrolet V8 454 cu. in. displacement, emissions certified for heavy-duty use in California and EPA.
Horsepower-215 @3,400rpm Torque - 332 ft. lbs. @
	3.400 rpm.
Isuzu 6 cylinder turbocharged
353 cu. in. displacement. Horsepower -160 @ 3200 rpm Torque - 289 ft. lbs. @
	2000 rpm.
3-speed turbo hydramatic with transmission oil cooler. Ratios:
1st gear 2.48 to 1
2nd gear 1.48 to 1
3rd gear 1.0 to 1
	Reverse 2.08 to 1
Morse Borg-Warner (Chevrolet with 1: 1.11 ratio) Diesel 1: 1 ratio.
Dana Model 70 axle with 3.73: 1 ratio. With engine and transmission in high gear, final ratio is 3.35 (Chevrolet); 3.73 (Diesel).
63 U.S. gallons capacity. Certified to CA Air Resources Board of Emissions Compliance.
Heavy-duty cross flow, with integral engine and transmission intercoolers.
12-volt negative ground systems.
Wiring: Heavy-duty all wiring is modern vinyl-insulated stranded copper, run in loom or as cable to prevent chafing. Combination circuit breaker system and fuse system.
500 cold cranking Amps maintenance free.
AL TERNATOR:
60 amp (as supplied with GM . engine).
INSTRUMENTS:
Non-glare reflective. Includes the following: 1. Speedometer 2. Tachometer. 3. Fuel Gauge. 4. Water Temperature Gauge. 5. Voltmeter. 6. Oil Pressure Gauge. 7. Vacuum Gauge. 8. Transmission Temperature Gauge.
WARNING SYSTEMS:
Included: 1. Parking Brake Warning Light. 2. Brake Failure Sentinel Light. 3. Turn Signal Indicators. 4. High Beam Indicators. 5. Emergency Flashers.
BODY Specifications:
Body Shell - Monocoque riveted aircraft aluminum structure
Frame & Stringers - Heat-treated, stretch-formed alum inum.
Exterior Skin - Heat-treated, high-tensile strength, loadbearing aircraft aluminum.
Floor - 3/4" exterior 5-ply fir, grade A-C. Sealed and waterproofed on the bottom and edges.
Heating System - Automotive-type, rated at 16,000 BTU's, with three-speed fan.
Bumpers - Front and rear wrap-around bumpers at 20-inch height.
Windshield - 1/4-inch laminated safety plate glass meets SAE standards.
Windshield Washers - Electric operated, with reserve reservoir.
Windshield Wipers - Two (2) heavy-duty electric-powered wipers.
Engine Service Access - There is a service hatch over the engine, next to the driver that is detachable for engine service, and a front engine access hood for checking fluid levels and minor service items.
Horn - Dual 12-volt, circuit breaker protected.
Exterior Lighting - Includes headlights, clearance lights, taillights, stoplights, marker lights, back-up lights, emergency flashers, turn signal lights, and reflectors.
Mirrors - All mirrors meet federal and SAE specifications. A convex high-visibility mirror is provided for additional safety.
7
--=