DOCUMENTATION AND OTHER VENDOR REQUIREMENTS FOR UPS UNINTERRUPTABLE POWER SUPPLIES

ELECTRICAL SAFETY REPORT COVERING:

AS 62040.1.1:2013
Uninterruptible power systems (UPS) - General and safety requirements for UPS used in operator access areas

AS/NZS 62368.1:2022
Audio/video, information and communication technology equipment - Part 1: Safety requirements (replaces earlier AS/NZS60065 and 60950 standards).

EMC REPORT COVERING:

AS/NZS CISPR 32:2015
Electromagnetic compatibility of multimedia equipment - Emission requirements
This supersedes both AS/NZS CISPR13 and AS/NZS CISPR22
This is required for the main product. If a plugpack power supply is bundled with it, then either the CISPR32 report should include that adaptor, or a separate report be supplied for the adaptor.

OTHER MANDATORY REQUIREMENTS:

CORD
Current Australian Approvals Certificates are required for: 
• The mains cord
• The mains plug 
• The appliance connector (if a detachable cord is used). 
Note that this is IN ADDITION  to the Approval Certificate for the appliance itself, if applicable.

• The components of the cord must be marked in accordance with the requirements of their approval certificates.
• The length of cords supplied in production product must match the length of the evaluated sample.

