DOCUMENTATION AND OTHER VENDOR REQUIREMENTS FOR USB FLASH DRIVE

EMC REPORT COVERING:

AS/NZS CISPR 32:2015
Electromagnetic compatibility of multimedia equipment - Emission requirements
This supersedes both AS/NZS CISPR13 and AS/NZS CISPR22
This is required for the main product. If a plugpack power supply is bundled with it, then either the CISPR32 report should include that adaptor, or a separate report be supplied for the adaptor.

OTHER MANDATORY REQUIREMENTS:

PSI-GEN
Pre-Shipment Inspection: Standard Checking Requirements for All Products
1. Factory address of PSI location MUST match address shown on initial Brief. (Critical Failure). Inspectors must take reasonable steps to verify that goods Inspected were actually made on those  premises.
2. GB internal packing must match specification (ie styrfoam, recycled fibreboard etc) and products must survive specified-height  drop test of outer carton, without obvious damage to product Giftbox.
3.  Labelling of outer carton must match supplied Data
4. Artwork of giftbox must match supplied artwork
5. Packed IM must match supplied Artwork
6. Warranty information either in manual or as separate document must match supplied documentation /artwork.

KNOWN CUSTOMER SATISFACTION ISSUES (FROM PAST EXPERIENCE):

FLASH MEMORY
• All flash memory devices  speed and Class claims must be suported by documentary evidence.
• All packaging and instructional material must clearly state that formatted capacity  is always going to be less than physical capacity. A minimum expected formatted size must be quoted.

MANUAL
USER MANUALS.
• All instruction manuals must be in clear, grammatically correct English. If required by QA, factory manuals must be re-written by a specialist manual authoring company.
• Fonts must be no smaller than 6 Point Arial, and must be easily readable by a person with normal vision, or using their normal reading glasses. That is, no additional magnification should be required to read the manual.
• All mandatory warning statements as required by the relevant safety standard must be included in the manual.
NOTE: Contrary to common belief, these do NOT have to be a word-for-word recitation of what is written the  the Standard; it is permissible to modify them to more accurately describe the particular product.
• A copy of the current Group Warranty Statement must be included in the  "Warranty" section. Take care to ensure that division contact details are correct. (For example, don't put Variety Store details in a Supermarkets product warranty).

