DOCUMENTATION AND OTHER VENDOR REQUIREMENTS FOR TOY SAFETY GENERAL

OTHER MANDATORY REQUIREMENTS:

AS/NZS ISO 8124.1:2023
Safety of toys 
Part 1: Safety aspects related to mechanical and physical properties (ISO 8124-1:2009, MOD)
This standard applies to all toys, i.e. any product or material clearly intended for use in play by children under 14 years of age.

Or:
EN71.1:2014
 Safety of toys - Part 1: Mechanical and physical properties
 

AS/NZS ISO 8124.3:2021
Safety of toys (safety requirements) 
Part 3: Migration of certain elements requirements. 
Specifies maximum acceptable levels and methods of sampling, extraction and determination for the migration of the elements antimony, arsenic, barium, cadmium, chromium, lead, mercury and selenium from toy materials and from parts of toys. It does not apply to packaging materials are not included, unless they are intended to be kept, for example boxes and containers, or unless they form part of the toy or have intended play value.

Or:
EN71.3:2013+A1
Safety of toys - Part 3: Migration of certain elements. 
This refers to banned substances used in paint and similar materials (eg lead, cadmium)

AS/NZS 8124.9:2008
Safety of toys Part 9: Organic chemical compounds 
For toys or  toy-like items intended or likely to to be placed in contact with the mouth or other sensitive body parts.

