DOCUMENTATION AND OTHER VENDOR REQUIREMENTS FOR GARDEN TOOLS

OTHER MANDATORY REQUIREMENTS:

GARDEN TOOLS
Details of the following testing is required. (Either in-house or from external testing)

• 24 hour 5% salt spray corrosion resistance
• Pull test for plastic handles and similarly stressed items
• UV resistance of any exposed plastic parts.
• Metal hardness
• Maximum cutting diameter (using wooden dowels)

