DOCUMENTATION AND OTHER VENDOR REQUIREMENTS FOR WIRELESS MICE AND KEYBOARDS

EMR REPORT COVERING:

AS/NZS 4268:2017+A1
Radio equipment and systems - Short range devices - Limits and methods of measurement .
(Basically, this is required by anything that uses a radio transmitter).

Note: If a product can also be used without the transmitter, it will need also need an EMC report to cover non-remote operation.
Understand the difference:
• EMC (ElectroMagnetic Compatibility)  reports are for devices that are NOT INTENDED to emit any electromagnetic radiation at all.
• Radiocommunications reports are for devices that are SPECIFICALLY INTENDED to produce electromagnetic radiation, (eg radio transmitters) but it must be strictly restricted to the licenced frequency.

OTHER MANDATORY REQUIREMENTS:

PSI-GEN
Pre-Shipment Inspection: Standard Checking Requirements for All Products
1. Factory address of PSI location MUST match address shown on initial Brief. (Critical Failure). Inspectors must take reasonable steps to verify that goods Inspected were actually made on those  premises.
2. GB internal packing must match specification (ie styrfoam, recycled fibreboard etc) and products must survive specified-height  drop test of outer carton, without obvious damage to product Giftbox.
3.  Labelling of outer carton must match supplied Data
4. Artwork of giftbox must match supplied artwork
5. Packed IM must match supplied Artwork
6. Warranty information either in manual or as separate document must match supplied documentation /artwork.

IP
Be aware of Intellectual Property issues and traps. Examples are Patents on White LEDs, Rovicorp's acquisition of a range seemingly trivial but potentially costly features of on-screen displays for Set Top Boxes, VCRs etc.
Also, all digital Video and Audio licensing must be in place (eg MPEG, MP3 etc)

KNOWN CUSTOMER SATISFACTION ISSUES (FROM PAST EXPERIENCE):

MANUAL
USER MANUALS.
• All instruction manuals must be in clear, grammatically correct English. If required by QA, factory manuals must be re-written by a specialist manual authoring company.
• Fonts must be no smaller than 6 Point Arial, and must be easily readable by a person with normal vision, or using their normal reading glasses. That is, no additional magnification should be required to read the manual.
• All mandatory warning statements as required by the relevant safety standard must be included in the manual.
NOTE: Contrary to common belief, these do NOT have to be a word-for-word recitation of what is written the  the Standard; it is permissible to modify them to more accurately describe the particular product.
• A copy of the current Group Warranty Statement must be included in the  "Warranty" section. Take care to ensure that division contact details are correct. (For example, don't put Variety Store details in a Supermarkets product warranty).

