DOCUMENTATION AND OTHER VENDOR REQUIREMENTS FOR INVERTER PORTABLE

ELECTRICAL SAFETY REPORT COVERING:

AS/NZS 4763:2011
Safety of portable inverters 
This Standard applies to single-phase or polyphase, air-cooled (natural or forced) portable inverters having a rated supply voltage not exceeding 60 V ripple-free d.c. and an alternating current (a.c.) output where: - the rated output does not exceed 3 kVA; - the rated output voltage is within the range 50 - 500 volt a.c; - the rated frequency of the output is within the range 40 - 100 Hz.

EMC REPORT COVERING:

AS CISPR 11:2017
Industrial, scientific and medical equipment - Radio-frequency disturbance characteristics - Limits and methods of measurement.

OTHER MANDATORY REQUIREMENTS:

CIG LIGHTER
Plugs intended to be fitted to car cigarette lighter sockets must be adequately rated for the current drain of the appliance.
If the internal fuse makes connection via a spiral spring, the spring must have sufficiently low electrical resistance to carry the maximum operating current without overheating. Generally, suitable springs are copper-plated and have the characteristic reddish colour.
A chrome- or stainless steel-finished spring is likley to have too much resistance and is only suitable for low-current devices.. Ideally the fuse holder will be designed  so that the current does not pass through the spring at all.

