Program: SJV2DSC
----------------
Runs on a PC only.

Input:	 A raw sysex file containing a single patch from the JV-1080
	 (or SUPER-JV). This file should be 643 bytes long.

Output:  A description (text) file with extension .dsc that contains a
	 readable description of all the patch parameter values.
	 It's easy to see the different values and to compare the 4 tones.

Syntax:  SJV2DSC <input-file(s)> [/s]
Option:  /s if you want the sysex headers/footers included in the .dsc file.

Example: SJV2DSC PIANO2.SJV
	 SJV2DSC PATC*.SJV

Author:  Geir Kilsti, Arendal, Norway
	 email: etogek@etn.ericsson.se

Any comments, suggestions or bug reports are welcome.
If you report a bug, please inlude the sysex-file and the .dsc file.

