Patchname       : Bright Lead 
Author          : Lance Ware (73114.753@compuserve.com)
UnitID          : 17
Dump Type       : Temporary Dump
Expansion Board : None
PCM Card        : SO-PCM1-02 (Guitar and Brass)

Description     : This is a medium-fat brassy patch for leads. It uses
                  3 tones. Tone 3 uses a soft trombone wave from the  
                  Guitar and Brass PCM card. If you don't have that, you
                  you can substitute something similar. Both Modulation 
                  and Expression affect the quality of the sound.
