Networking Essentials - Memory Sheet

IRQ # | Common Use | I/O Address
IRQ 1 |  |
IRQ 2(9) |  |
IRQ 3 |  | ____________
IRQ 4 |  | ____________
IRQ 5 |  |
IRQ 6 |  |
IRQ 7 |  |
IRQ 8 |  |
IRQ 9 |  | ____________
IRQ 10 |  |
IRQ 11 |  |
IRQ 12 |  |
IRQ 13 |  |
IRQ 14 |  |
IRQ 15 | _______________________________________ |

What four things do you need to configure for an adapter card install?

1

2

3

4

IBM Cabling

Type 1 |  | 2-pair 22AWG | used for computers and MAU's.
Type 2 |  | 2-pair 22AWG + pair 26 AWG for voice |
Type 3 |  | 4 solid, unshielded twisted pair 22 or 24 AWG |
Type 5 |  | 2 fibers | industry standard
Type 6 |  | 2-pair 26 AWG |
Type 8 |  | 2-pair 26 AWG | Limited to 1/2 the distance of Type 1 cable
Type 9 |  | 2 STP cables |

802 Project Model

802.1 |
802.2 |
802.3 |
802.4 |
802.5 |
802.6 |
802.7 |
802.8 |
802.9 |
802.10 |
802.11 |
802.12 |
| _____________________________________________________

Access Methods

Feature or Function | CSMA/CD | CSMA/CD | Token Passing | Demand Priority
Type of Communication |  |  |  |
Type of Access Method |  |  |  |
Type of Network |  |  |  |

Comments and suggestions? E-mail me at grantwil@sk.sympatico.ca
Last Updated: Wednesday, March 10, 1999 | Grant Wilson, Tisdale, SK. Canada