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	Methods of rigging spinnaker gear on Corsairs vary, from boat to boat as do types of fittings used by each skipper.

This list is intended as a guide to help boat owners and is the most common method used. 

Click on the hardware photo to get more info on item.

	

RONSTAN website click on the logo above

HALYARD GEAR

Mast Diagram


Various Control Boards
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Spinnaker halyard
35 feet or 10.67 metres long, 6mm dia. Pre stretched 100% Braided polyester rope.



To attached the Saddle or Kite Block. 

See Mast Diagram
24. From the highest effective point of the spinnaker halyard fitting over which the spinnaker halyard will pass to the extremity of the mast foot casting
Measurement; 
Ft. ins 15'11-7/8", 4874 mm.
Tolerance + 0'0-3/8"Ft. ins + 10 mm, Ft. ins - 0'0-3/8" - 10 mm.
24. A The spinnaker halyard must leave the halyard fitting at a point no more than 3" (76 mm) from the front of the mast and then lead directly to the head of the spinnaker.

Measurement; 

0'3" Ft. ins, 76 mm

Tolerance + 0" Ft. ins, + 0 mm. - 3" Ft. ins, - 76 mm.
External Halyard

RF467 Block for halyard on mast & SS saddle for pulley.
Single, swivel shackle head, Series 29mm 




          



To have a trouble free spinnaker, place a small pulley on the centerboard.
Internal halyard

2 Exit block RF 20711 & RF 20711A.
When the hole is drilled for Kite Block, attached a sinker to end of halyard. Place the mast on an angle, insert the halyard with sinker in the top hole of mast and lower the halyard to the bottom of mast. Use a coat hanger to retrieve it. Attached the Exit block RF 20711A, then the cover plate RF 20711.



Head & Foot of Spinnaker

Use a bowline to tie the halyard to the spinnaker, or a Flag Clip with swivel RF532 can be used.


Centreboard
A RF30140 block can be used to guide the spinnaker halyard from the mast to the tabernacle. Series 30 mm. See photo above.


Control Board
Block RF 30151A on tabernacle for halyard. Series 30 mm. 



Cam cleat RF 510 on Control Board for halyard 
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