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	Methods of rigging mainsheet gear on Corsairs vary, from boat to boat as do types of fittings used by each skipper.
This list is intended as a guide to help boat owners and is the most common method used.

Click on the hardware photo to get more info on item.

	336 Deciduous[image: image1.jpg]- .
rﬁyﬁ'ﬂg g Corsazz B
Li :x ,





	

RONSTAN website click on the logo above
To attached stainless steel boom hangers to a boom
See Boom Diagram.
32. From the front of the boom to the centre of the first mainsheet attachment point.
Measurement; 4'4" Ft ins, 1321mm.

Tolerance; + 0'1" – 0111 Ft. ins, + 26 mm. – 0111” Ft. ins, – 26 mm.

33. From the front of the boom to the centre of the second mainsheet

attachment point. 
Measurement 5'2" Ft ins, 1575 mm.

Tolerance; + 0'1"Ft. ins + 26 mm. - 011" Ft ins, - 26  mm.
34. Distance between mainsheet attachment points.
Measurement; 0'l0" Ft ins, 254 mm.
Tolerance; + 0'I" Ft ins, + 26 mm. - 0'1” Ft ins  - 26 mm.
36. From the mainsheet attachment points to the lower edge of the boom.
Measurement; 0'1" Ft ins, 26 mm.
Tolerance; + 0'0-1/4" Ft ins + 6.5 mm, - 0'0-1/4" Ft ins - 6.5 mm.


Boom Diagram


Wire Rope with a Thimble on each side

Attach a Wire rope to each boom hanger

Length 25cm includes thimbles. Wire diam. 1.5mm.
By using the wire hangers allows you to use less rope - therefore less rope to pull on and let out when adjusting the mainsail.



Mainsheet Boom Pulleys RF51100 

Series 50mm, All Purpose Blocks.
Single, universal head.


Mainsheet Centreboard Pulley RF51111

Series 50mm All Purpose Blocks.
Single, becket, loop head.


Mainsheet Block RF51530

Series 50mm. 

Fiddle, adjustable cleat, universal head.
Mainsheet Block RF50520

Ball bearings provide high performance & low friction. Series 50mm. 

Fiddle, adjustable cleat, universal head.


Mainsheet

Rope Diam 6 to 8 mm (3/8in), Length Coming soon  

Pre stretched 100% Braided polyester rope.


Tennis Ball

A Tennis Ball is a simple way of holding up the mainsheet block.
Make two nicks in the top and the bottom of the ball and painstakingly do up the shackle on the floor under the ball.




	

	

	More photo’s coming soon 
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