PRASAR BHARATI

(BROADCASTING CORPORATION OF INDIA)

OFFICE OF THE CHIEF ENGINEER (SZ)

ALL INDIA RADIO & TELEVISION

CHENNAI-600 005

No.CESZ/SMT/GD-Tech/2006                            

Date: 26-6-06

Circular

Sub: Spares for Harris 10 KW FM Transmitter - Reg

Ref: Ban-2/6/2K6/E dated 13-6-2006

Sir/ Madam,      


             Indigenous replacement for Harris Transmitter spares for contactors, relays & Stock spares before a real emergency arises : Letter in this connection received from AIR Bangalore is enclosed for necessary action.

                         It has been observed that the PCB boards having MOVAR devices are failing frequently at stations & likely to cause a long breakdowns / consume time for replacement. Hence the stations may kindly keep enough number of fabricated PCB boards with MOVAR for ready use in circuits. 

 Yours faithfully,

   B. MUTHULAKSHMI.

ASST. ENGINEER

For Chief Engineer ( SZ )

Copy to,

Engineering Heads of all AIR stations in South Zone
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To 6 })}}/
‘/C{:ief Engineer (S7) CL
(By name Sri G. Natarajan, DSM) }’}/

All India Radio & TV

Swami Shivananda Salai (O
Chennai 600005. )\;A\ S
Dear Sir,

This is in continuation of this office letter of even number dated 31.3.2006 reporting
about the failure of 3 phase power contactor of Harris 10KW FM transmitter-Z10 (Part
No.5700372000 Make Furnas 42GE 35 ALlO@S’mps, 3 polé) of both RAINBOW and
Vividh Bharati channels of this station. The failure was probably due to wear and tear of
the contactor as it has to operate every time the transmitter is switched ON/OFF. Station
also reported that it is not possible to replace this imported contactor by indigenous one
due to space constraints inside the transmitter cubicle. Hence it (a5 decided that the
defective contactor esmpenents is to be replaced only by the original Furnas make
confactor. All these days station some how could run the tranmitter by making some
temporary repairs to the contactor contacts.

The spare part was not available with Station Engineer, Central Stores, New Delhi.
Hence efforts were made by the station to procure the components either from the local
market or from M/s. Horizon Broadcast Electronics, Gurugaon, the authorized distributor
of Harris as suggested by Zonal office. However it is found that the price quoted by
authorized dealer of Harris was Rs.50000+Tax per contactor. As the rate was exorbitantly
high, efforts were made by the station to source the component directly from Furnas
(presently taken over by M/s. Siemens). The source was located some whete in Germany
and the contactor was imported through the local supplier at the rate of Rs...26000 per
unit +freight +Tax. 2 numbers of contactors have been procured during last week and-t-
hals been taken into circuit immediately. Both the contactors are working satisfactorily

During replacement of the contactor it was noticed that the associated MOV AC
protector board of the contactor (Part No 992-8553-005) was defective due to failure of
couple of MOV components and also the PCB boards was damaged due to arcing. As the
replacement board was not available with the station, similar PCB board was got
fabricated and assembled with the suitable locally available model to meet the
requirement. This board is also taken into circuit and is working satisfactorily since last
one week.
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My
uperintending Engineer

For kind information,

Copy to:

1. Director General (By name Sii G.I.. Kawatra, DE(TM)), AIR, Akashvani Bhavan,
New Delh 110 001.

2. Station Engineer, Central Stores, All India Radio, 14-B, LP. Estate, Ring road,
New Delhi 110002,

Superintending Engineer




