CARS NET PREAMBLE

Calling the CARS Net; Calling the CARS Net.  This is          
calling the Net of the Cascade Amateur Radio Society.  The purpose of this net is for passing traffic, preparing amateurs for communication in the event of an emergency and to provide those with a common interest the opportunity to meet. This is a directed net.  Please follow the direction of net control.  Do not attempt to relay, unless asked to do so by net control.  Stations checking in are requested to remain on frequency until all traffic has been assigned and net business has been completed.  This net will accept emergency traffic at any time.  Should it be necessary to leave the net, please check out with net control.  Although primarily for members of the Cascade Amateur Radio Society, all amateurs are invited to check into this net.  This net meets every Sunday at 21:00 Pacific time on 147.56MHz. This net is held in conjunction with an HF NET on 3965KHz every Monday night at 21:00, conducted by MARA Northwest. Net Control tonight is 
             , my name is                 and my station location is                     .

Is there any emergency traffic?	(Handle immediately as listed.)

The net is now open for check-ins.  Please check-in with your callsign, your name, your location, and any formal traffic by mentioning "with traffic". (Handle all check-ins alphabetically by callsign suffix: Alpha-Hotel, India-Lima, Mike-Romeo, Sierra-Zulu)

Are there stations with Bulletins?   (Handle immediately after all are listed)

Are there any stations with formal traffic? (Only one on the net frequency.)

We’ll now go through the check-ins in round-table fashion:
(brief synopsis of each)

Call Sign		Comments

(After completion of listed round table)
This is         , Calling for any late check-ins.

(Acknowledge and allow an opportunity for comments at the same time)

I would like to thank all check-ins to the Net of the Cascade Amateur Radio Society.  Should an emergency arise, all members are requested to tune to this frequency, 147.56MHz, and/or the HF Frequency 3965KHz.  147.58MHz is the designated secondary frequency for this net.  This is             closing this session of the Cascade Amateur Radio Society Net and releasing the frequency to general amateur use. Have a good evening.