Pilot Series Checklist Boeing 767-300 Full Version for FS2000
Component of The Pilot Series Checklist Part IV
Made by Chris van Bijlert
http://fly.to/pilotserieschecklist

____________________________________
      COCKPIT PREPARATION
____________________________________
Cockpit Initial Preparation

- Battery Switch: ON (GUARDED)
- Standby Power Selector: AUTO
- Gear Handle: DOWN and IN
- Flap Handle/Indicator: AGREE
- APU: START
- APU Power/External Power: ESTABLISH
- Pneumatics and Airconditioning: ESTABLISH
- Exterior Lights: CHECK
- Transponder: SET
- Parking Brake: SET

- Cockpit Initial Preparation: COMPLETED

____________________________________
Cockpit Final Preparation

- Yaw Damper Switches: CHECK/AS REQUIRED
- Caution Annunciatior Panel: CHECK
- Standby Power: TEST/AUTO
- Engine Start Panel: SET/CHECK
- Fuel Panel: CHECK
- Wing Anti-Ice Switch: BLANK
- Engine Anti-Ice Switches: BLANK
- No Smoking Signs: ON
- Fasten Seat Belts Signs: OFF
- Standby Instruments: CHECK
- Caution and Warnings: CHECK
- Standby Engine Indicators: AUTO
- Auto Brakes Selector: OFF
- Engine Oil Quantity: CHECK
- EICAS/ENGINE Display: CHECK
- Spoiler Handle: DOWN
- Throttles: CHECK
- Stabilizer Trim: SET/CHECK
- Fuel Control Switches: CUTOFF
- Fuel Panel, QTY, Distrib: SET AND CHECK

- Cockpit Final Preparation: COMPLETED

____________________________________


____________________________________
	NORMAL PROCEDURES
____________________________________
Before Starting Engines Checklist

- Rudder Pedals/Seat: ADJUST/LOCKED
- Fuel Panel/Quantity: SET/()LBS AND CHECKED
- No Smoking Signs: CHECK ON
- AFDS Panel: SET/CHECKED
- FLT Instr Switches and Bugs: SET/CHECKED
- EICAS Status: CHECK
- Gear Handle and Lights: DOWN/GREEN
- Flaps: UP
- Throttles: CLOSED
- Fuel Control Switches: CUTOFF
- Spoiler Handle: DOWN
- Brakes: PARKED
- NAV Radios/TRNSP: SET

Before brake release or engine start:
- Seat Belt Signs: ON
- Fuel Pumps: ON
- Red Anti-Collision Lights: ON
- Packs: OFF

- Before Starting Engines Checklist: COMPLETED

____________________________________
Taxi Checklist

- Left and Right ISLN Valves: CLOSED
- Packs: ON
- Engine Anti-Ice: AS REQUIRED
- APU: AS REQUIRED
- Flaps: DOWN
- Flight Controls: CHECKED
- EICAS Display: RECALL/CHECK
- Fuel Panel: CHECK

- Taxi Checklist: COMPLETED

____________________________________
Before Takeoff Checklist

- T/O Data and Bugs: REVIEWED
- AFDS/Radios: SET
- Stab Trim: SET
- Flaps: SET
- EICAS: RECALL/CANCEL
- Anti-Ice: AS REQUIRED
- Packs: AS REQUIRED
- Auto Brake Selector: RTO
- Landing Lights: ON

- Before Takeoff Checklist: COMPLETED

____________________________________
After Takeoff Checklist

- Gear: NO LIGHTS/OFF
- Auto Brake Selector: CHECK OFF
- White Anti-Collision Lights: ON
- Packs: ON
- Flaps: UP
- No Smoking Signs: AS REQUIRED

At 18,000 feet MSL:
- Altimeters: RESET/CHECKED
- Landing Lights: CHECK OFF

- After Landing Checklist: COMPLETED

____________________________________
Descent Checklist

- Fuel Panel/Crossfeed: AS REQUIRED
- Engine and Wing Anti-Ice: AS REQUIRED
- Landing Data: REVIEWED

Descending thru FL180 or leaving cruise:
- Altimeters: RESET/CHECKED
- Landing Lights: ON

- Descent Checklist: COMPLETED

____________________________________
Before Landing Checklist

- Altimeters: SET
- AFDS/Radios: SET
- FLT Instr and Bugs: SET
- Seat Belt/No Smoke: ON
- EICAS: RECALL/CANCEL
- Gear: DOWN
- Auto Brake Selector: AS REQUIRED
- Spoilers: DOWN/ARM
- Flaps: SET

- Before Landing Checklist: COMPLETED

____________________________________
After Landing Checklist

- Autopilots/Autothrottle: OFF
- White Anti-Collision Lights :OFF
- Flaps: UP
- Spoiler Handle: DOWN
- Landing Lights: OFF
- APU: AS REQUIRED

- After Landing Checklist: COMPLETED

____________________________________
Parking Checklist

- Brakes: PARKED
- Seat Belt Signs: OFF
- APU or External Power: ESTABLISHED
- Left and Right ISLN Valves: OPEN
- Fuel Control Switches: CUTOFF
- Red Anti-Collision Lights: OFF/AS REQUIRED
- Auto Brake Selector: OFF
- Fuel Pumps: OFF
- Wing Anti-Ice: OFF
- Engine Anti-Ice: OFF
- Packs: AS REQUIRED
- Recirculation Fans: AS REQUIRED

If leaving aircraft:
- APU: AS REQUIRED
- Standby Power: AS REQUIRED
- Battery Switch: ON or OFF IF NO EXT OR APU PWR

- Parking Checklist: COMPLETED

____________________________________


____________________________________
	IMPORTANT NOTES
____________________________________
* The Pilot Series Boeing 767-300 Checklist Full Version for FS2000. 

* Checklist for Boeing 767-300 made by Chris van Bijlert.
  Can also be used on Boeing 767-200.
  Derived from Eric Ernst's 757/767 panel.
  Visit The Official Pilot Series Checklist Website: 
  http://fly.to/pilotserieschecklist
  Email me: chrisvanb@geocities.com

* Feel free to upload this checklist along your own
  freeware aircraft, as long as you limited it to one single 
  aircraft at a time. If you want to use this checklist on
  more than one aircraft at a time please contact me. 
  But do always keep this piece of text on it 
  and credit the designer (me!).
  When downloading and using this checklist you automaticly 
  agree with the Copyright & Use Notice as stated in the 
  documentation and on the website.

* Copyright (C.) Chris van Bijlert and Eric Ernst.