Preparing a Safe Room
Extreme windstorms in many parts of the country pose a serious threat to buildings and their occupants. Your residence may be built “to code,” but that does not mean it can withstand winds from extreme events such as tornadoes and major hurricanes. The purpose of a safe room or a wind shelter is to provide a space where you and your family can seek refuge that provides a high level of protection. You can build a safe room in one of several places in your home.
•	Your basement. 
•	Atop a concrete slab-on-grade foundation or garage floor. 
•	An interior room on the first floor. 
Safe rooms built below ground level provide the greatest protection, but a safe room built in a first-floor interior room also can provide the necessary protection. Below-ground safe rooms must be designed to avoid accumulating water during the heavy rains that often accompany severe windstorms.
To protect its occupants, a safe room must be built to withstand high winds and flying debris, even if the rest of the residence is severely damaged or destroyed. Consider the following when building a safe room:
•	The safe room must be adequately anchored to resist overturning and uplift. 
•	The walls, ceiling, and door of the shelter must withstand wind pressure and resist penetration by windborne objects and falling debris. 
•	The connections between all parts of the safe room must be strong enough to resist the wind. 
•	Sections of either interior or exterior residence walls that are used as walls of the safe room, must be separated from the structure of the residence so that damage to the residence will not cause damage to the safe room.