# Data Link Simulator Log:

Flow Control | %flow_control%
Error Detection | %error_detection%
Error Control | %error_control%

Frame Size | %frame_size%
Window Size | %window_size%
Randomise Error | %randomise_error%

Message to Send | %message%

Sender | Receiver
    %sender_log%
    %receiver_log%

## Legend:

- FCS - Frame Check Sequence, CRC bits append to data
- RR - Receive Ready, analogous to positive acknowledgement (ACK)
- RNR - Receive Not Ready
- REJ - Reject, analogous to negative acknowledgement (NACK) in Go Back N ARQ
- SREJ - Selective Reject, analogous to negative acknowledgement (NACK) in Selective Reject ARQ