	Prussick or Prussik
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Also called Double Lark's head.  A very useful knot. If made in the end of a line this knot is a fixed loop, which you easily can resize, just by moving the knot. Suitable as a guy-line knot.
Tying the Prusick with only one final loop, instead of two (making 3 turns around the standing part rather than 4) is called a "taut line hitch" and serves the same purpose as the Prusick. Used by scouts to keep guy ropes taut on tents and towers. Very useful.
Normaly the prussick is made with a thin line on a rope. This thinner line could then be used as a handle that could be moved on the rope. James Bond used his shoelaces in a movie to climb a rope using this knot.
	Lark's head
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Very easy to do, it can be done even if both ends are tied. Both ends should have the same load; otherwise it will not be reliable. Use it when you want to tie a tarpaulin, where the holes exist.

	Fisherman's Loop
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A fixed loop. Quick to make. The name of the knot comes from the time when the fishermen could not write. Instead of a handwritten letter, the fisherman sent this knot home to his fiancée, with the two knots a bit separated. If it came back with the knots together, the answer was... YES!
	Jug Sling Hitch
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A very useful knot. In swedish it is called 'sack-knot from England', because the mealers used this knot to tie toghether the sacs. The loop is a useful handle, or you can use it as a hanger.

	Fisherman's Knot
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For stiff ropes and cords you shall use the Fisherman's Knot. Easy to make, dificult to untie, so don't use it on a good rope, especially if there is a lot of strain on it. You should make it double on cords of nylon, or it will not last.
	Vice versa
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Vice versa is also a variant of sheet bend and square knot.


	Water Knot
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A third knot for tying two ropes of the same thickness. Very strong knot, but difficult to untie. Good for tying grasses, wet rope, and rubber together (e.g. for repairing swimming goggles).
	Simple Simon Over
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Simple Simon Over is a variant of a square knot. Start as when doing a sheet bend with a loop.

	
	Simple Simon Under
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Not very different from Simple Simon Over, but is a little more secure.

	
	

	
	

	
	

	
	

	
	


