Making Bush Shirts P2

The armhole is cut using a template. The cut is about 4cm deep and varies across the diagonal according to the size of the shirt.

The bottom of the shirt can be rounded off to make 2 tails with the front of the shirt shorter than the back, or it may be left square for the moment, as has been done here.

The pocket is cut with a wedge-shaped top that sandwiches over the flat rectangular panel. There are other ways of doing the patch pocket.