Making Bush Shirts 6

The front panel of the shirt should look like this. Cut a slit from the base of the collar about 12 inches, or 30cm.

This makes the slit for the front placket. On the shirt, it should be just above the navel,

When the shirt is folded out and laid out flat, the basic design can be seen. It is not necessary to make a special cut at the base of the slit. The placket front is actually easier to make than a polo front.