Setting in sleeves

| Lay shirt down, fair side of fabric up. Place sleeve on top, positioning centre of sleeve top on sleeve inset join, rough side of fabric up.

| Sew one side of sleeve first, then the other, so that the sleeve is correctly placed in the armhole.

| Turn correct side out. Trim off excess if necessary. Turn inside out. Seam along arm and down one side. If shirt has front and back tails, sew a seam around the tails to seal off fabric.